For 1990-2009 cars

## Battery Usage Gasoline Engines

Application | Specification
--- | ---
Metric | English
Cold Cranking Amps | 610 Amps
Cold Cranking Amps - Extremely Cold Area | 610 Amps
Load Test | 300 Amps
Minimum Voltage | Estimated Temperature

- 9.6

21°C

69.8°F

- 9.5

15.6°C

60°F

- 9.4

10°C

50°F

- 9.3

4.4°C

40°F

- 9.1

-1.1°C

30°F

- 8.9

-6.7°C

20°F

- 8.7

-12.2°C

10°F

- 8.5

-17.8°C

0°F

Reserve Capacity Minimum | 90 minutes

## Battery Usage Diesel Engine

Description | Specification
--- | ---
Unit | Standard
Type | -- | Maintenance Free
Output (Capacity) | V-AH | 12V-90AH
Cold Cranking Amps (CCA) | CCA | 912
Load Test | amps | 450
Minimum Voltage

- 9.6

V

21°C (70°F) and above

- 9.5

V

15.6°C (60°F)

- 9.4

V

10°C (50°F)

- 9.3

V

4.4°C (40°F)

- 9.1

V

-1.1°C (30°F)

- 8.9

V

-6.7°C (20°F)

- 8.7

V

-12.2°C (10°F)

- 8.5

V

-17.8°C (0°F)