For 1990-2009 cars

## Exhaust Gas Recirculation Valve Replacement European and North American Emissions

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the vacuum hose from the exhaust gas recirculation (EGR) valve.
3. Remove the EGR valve retaining bolts.
4. Remove the EGR valve from the electronic ignition (EI) system ignition coil adapter.

### Installation Procedure

1. Clean the EI system ignition coil adapter mating surface.
2. Install the new EGR valve gasket.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the EGR valve with the bolts.

Tighten
Tighten the EGR valve retaining bolts to 30 N·m (22 lb ft).

4. Connect the vacuum hose to the EGR valve.
5. Connect the negative battery cable.

## Exhaust Gas Recirculation Valve Replacement Non European Emissions

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the vacuum hose from the exhaust gas recirculation (EGR) valve.
3. Remove the EGR valve retaining bolts.
4. Remove the EGR valve.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the EGR valve with the bolts.

Tighten
Tighten the electrical EGR valve retaining bolts to 30 N·m (22 lb ft).

2. Disconnect the vacuum hose to the EGR valve.
3. Connect the EGR valve electrical connector.
4. Connect the negative battery cable.