For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug | 12 N·m | 106 lb in
Adjuster Plug Locknut | 75 N·m | 56 lb ft
Air Filter Housing Assembly Bolts | 6 N·m | 53 lb in
Control Module Bracket Bolts | 7 N·m | 62 lb in
Dash Seal Retaining Ring Nuts | 7 N·m | 62 lb in
Fluid Reservoir | 10 N·m | 89 lb in
High Pressure Hose Fitting | 28 N·m | 21 lb ft
Hydraulic Cylinder Pipe Fittings -- Cylinder End | 28 N·m | 21 lb ft
Hydraulic Cylinder Pipe Fittings -- Valve End | 18 N·m | 13 lb ft
Inner Tie Rod | 100 N·m | 74 lb ft
Intermediate Shaft Pinch Bolts | 25 N·m | 18 lb ft
Outer Tie Rod Adjusting Nut | 64 N·m | 47 lb ft
Outer Tie Rod Nuts | 50 N·m | 37 lb ft
Pinion Locknut | 30 N·m | 22 lb ft
Pinion Preload | 1 N·m | 9 lb in
Power Steering Pump Bolts | 25 N·m | 18 lb ft
Power Steering Pump Pressure Pipe Fitting | 28 N·m | 21 lb ft
Pressure Pipe Retaining Clip Bolts | 8 N·m | 71 lb in
Radiator Clip Bolts | 8 N·m | 71 lb in
Return Pipe Clip Bolts | 8 N·m | 71 lb in
Right Side Power Steering Pump Bracket Bolts | 35N·m | 26 lb ft
Steering Gear Inlet and Outlet Pipe Fittings | 28 N·m | 21 lb ft
Steering Gear Mounting Bracket Nuts and Bolts | 60 N·m | 44 lb ft
Transaxle Center Bracket-to-Engine Bolt | 80 N·m | 59 lb ft