For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement Five Door/Wagon

### Removal Procedure

1. Remove the screws from the instrument cluster trim panel.
2. Remove the instrument cluster trim panel.

### Installation Procedure

1. Install the instrument cluster trim panel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the instrument cluster trim panel screws and tighten to 4 N·m (35 lb in).

## Instrument Cluster Trim Panel Replacement Four Door

### Removal Procedure

1. Remove the screws and the instrument cluster trim panel.
2. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the instrument cluster trim panel with the screws and tighten to 4 N·m (35 lb in).