For 1990-2009 cars

### Removal Procedure

1. Remove the interior garnish molding.
2. Remove the screws and the exterior garnish molding.
3. Remove the rear door secondary weatherstrip.

### Installation Procedure

1. Install the rear door secondary weatherstrip.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the exterior garnish molding with the screws.
3. Install the interior garnish molding.