For 1990-2009 cars

### Removal Procedure

1. Remove the theft deterrent alarm electrical connector.
2. Remove the theft deterrent alarm bracket mounting bolts and the theft deterrent alarm.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the theft deterrent alarm with the mounting bolts.

Tighten
Tighten the theft deterrent alarm bracket mounting bolts to 8 N·m (71 lb in).

2. Connect the theft deterrent alarm electrical connector.