For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the stabilizer shaft-to-stabilizer link nut.
4. Remove the stabilizer link-to-strut assembly nut.
5. Remove the stabilizer link.

### Installation Procedure

1. Install the stabilizer link.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer link-to-strut assembly nut.

Tighten
Tighten the stabilizer link-to-strut assembly nut to 47 N·m (35 lb ft).

3. Install the stabilizer shaft-to-stabilizer link nut.

Tighten
Tighten the stabilizer shaft-to-stabilizer link nut to 47 N·m (35 lb ft).

4. Install the wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.