For 1990-2009 cars

### Removal Procedure

1. Raise and properly support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Position an appropriate drain pan under the engine.
3. Remove the oil pan drain plug bolt.
4. Remove the oil filter.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil filter and tighten to 15 N·m (11 lb ft).
2. Discard the used oil pan drain plug washer and replace with a new oil pan drain plug washer.
3. Install the oil pan drain plug bolt and tighten to 35 N·m (26 lb ft).
4. Lower the vehicle.
5. Fill the engine with oil to the appropriate mark.
6. Start engine and inspect for leaks.