For 1990-2009 cars

Checks | Actions
--- | ---
Inspect for an external leakage of the power steering pump at the seals. |

1. Replace the seals.
2. Repair the leak.
3. Bleed the system.

Inspect for a worn serpentine accessory drive belt. | Replace the serpentine accessory drive belt.
Inspect the power steering pump for internal leaks. | Replace the power steering pump.
Inspect the hoses for damage or restricted flow. | Replace the power steering hoses and/or pipes.
Inspect the power steering fluid level. | Fill the power steering fluid reservoir.
Inspect the power steering pump flow control valve for sticking and improper operation. | Replace the power steering pump.