For 1990-2009 cars

1. Move the shift control lever into the neutral (N) position.

Important: The various shift control cable positions must match at the shift control lever in the vehicle and at the selector lever on the transaxle to provide proper transaxle shifting.

2. Loosen the control cable adjusting nut.
3. Put the transmission range (TR) switch lever in neutral (N).

Notice: Refer to Fastener Notice in the Preface section.

4. Pull the shift control cable until it is tight and tighten the control cable adjusting nut.

Tighten
Tighten the control cable adjusting nut to 8 N·m (71 lb in).

5. Install the floor console. Refer to Front Floor Console Replacement .