For 1990-2009 cars

#### Tools Required

DT 46475 (DW260-070) Auto Transaxle Oil Plug Remover/Installer

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Vehicle Lifting and Jacking Notice .
2. Place a fluid container below the fluid level plug.

Caution: When the transmission is at operating temperatures, take necessary precautions when removing the check/fill plug, to avoid being burned by draining fluid.

3. Using DT 46475 (1) remove the fluid drain plug.
4. Allow the transaxle fluid to drain.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Use the DT 46475 (1) to install the transaxle fluid drain plug.

Tighten
Tighten the drain plug to 45 N·m (33 lb ft).

2. Add the transaxle fluid. Refer to Transmission Fluid Level Inspection .