For 1990-2009 cars

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the clutch B/E. Refer to Clutch B/E Disassemble .
2. Remove the rear sun gear.
3. Remove the planetary gear set.
4. Remove the snap ring from the front ring gear.
5. Remove the planetary gear set.
6. Remove the axial needle bearing.
7. Remove the front gear set with the rear ring gear, the front sun gear, and the oil trays.
8. Remove the oil trays and the front sun gear from the planetary gear set.