For 1990-2009 cars

#### Tools Required

• | J 42960-2 Fuel Flapper Door Holder

• | J 42960-1 Fuel Drain Hose

Warning: Never drain or store fuel in an open container. Always use an approved fuel storage container in order to reduce the chance of fire or explosion.

Warning: Place a dry chemical (Class B) fire extinguisher nearby before performing any on-vehicle service procedures. Failure to follow these precautions may result in personal injury.

1. Remove the fuel filler cap.
2. Install the J 42960-2 into the fuel fill pipe in order to hold the door open.
3. Insert the J 42960-1 into the fuel tank until the hose reaches the bottom of the fuel tank.
4. Use an air operated pump device in order to drain as much fuel through the fuel fill pipe as possible.