For 1990-2009 cars

#### Tools Required

• | DT 46463 (DW240-150) Transaxle Case Side Bearing Outer Race Adapter

• | DT 46465 (DW240-170) Adapter Handle

1. Place the matchmarks (1) on the ring gear and differential case.
2. Remove the 8 bolts.
3. Using a plastic hammer, tap on the ring gear to remove it from the case.
4. Using a suitable puller, remove the tapered roller bearing of transaxle housing side.
5. Using a suitable puller, remove the tapered roller bearing of transaxle case side.
6. Using a pin punch and hammer, drive out the pin from the ring gear side.
7. Remove the differential pinion shaft from the case.
8. Remove the 2 differential pinion gears, 2 differential side gears, 2 differential pinion thrust washers, and 2 differential side gear thrust washers.
9. Using a driver, remove the oil seal from the transaxle housing.
10. Using a suitable puller, remove the side bearing outer race of transaxle housing.

Notice: Use extreme care not to damage the transaxle case when removing the oil seal using a screwdriver.

11. Using a driver, remove the oil seal of transaxle case.
12. Using the DT 46463 (2) and the DT 46465 (1), remove the transaxle case side bearing outer race and shim.