For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gages and Console.
3. Disconnect the control module/receiver electrical connector.
4. Slide the control module/receiver away from the mounting bracket.

### Installation Procedure

1. Install the control module/receiver on its mounting bracket.
2. Connect the control module/receiver electrical connector.
3. Install the floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gages and Console.
4. Connect the negative battery cable.