For 1990-2009 cars

### Removal Procedure

1. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
2. Remove the bolt and the upper front seat belt anchor.
3. Remove the upper portion of the lower center pillar trim panel.
4. Pry off the upper center pillar trim panel.

### Installation Procedure

1. Install the upper center pillar trim panel.
2. Install the upper portion of the lower center pillar trim panel to its original position.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper front seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).

4. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .