For 1990-2009 cars

### Removal Procedure

Note: The Left-Hand Drive is Shown. The Right-Hand Drive is Similiar

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel under cover. Refer to Knee Bolster Replacement.
3. Disconnect the electrical connector.
4. Remove the sensor retaining screw.
5. Remove the sensor.

### Installation Procedure

1. Install the sensor with the retaining screw.
2. Connect the electrical connector.
3. Install the instrument panel under cover.Refer to Knee Bolster Replacement.
4. Connect the negative battery.