For 1990-2009 cars

#### Tools Required

DT 46470 (DW260-030) Differential Oil Seal Installer

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the drive axles. Refer to Front Drive Axle Inner Shaft Replacement.

Important: Do NOT damage the bore of the transaxle case.

3. Remove the transaxle drive seal using a flat-bladed tool. If necessary, crush the seal first in order to loosen the seal from the case.

### Installation Procedure

1. Use DT 46470 (1) to install the transaxle drive seal.
2. Install the drive axles. Refer to Front Drive Axle Inner Shaft Replacement.
3. Connect the negative battery cable.