For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear compartment lock cover.
3. Disconnect the electrical connector.
4. Remove the screws and the rear compartment lock.
5. Disconnect the lock rod.

### Installation Procedure

1. Connect the lock rod.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear compartment lock with the screws.

Tighten
Tighten the rear compartment lock screws to 6 N·m (53 lb in).

3. Connect the electrical connector.
4. Install the rear compartment lock cover.
5. Connect the negative battery cable.