For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the tweeter speaker by prying the tweeter speaker out of the door trim panel.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the tweeter speaker into the door trim panel.
3. Connect the negative battery cable.