For 1990-2009 cars

#### Special Tools

DT 46475 (DW260-070) Auto Transaxle Oil Plug Remover/Installer

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil pan and the oil pan gasket with the bolts and tighten to 6 N·m (53 lb in).
2. Install the oil cooler inlet and outlet pipes. Refer to Transmission Fluid Cooler Hose/Pipe Replacement.
3. Use DT 46475 (1) to install the transaxle fluid drain plug.
4. Install the engine cover. Refer to Engine Cover Replacement.
5. Refill the transaxle fluid. Refer to Transmission Fluid Level Inspection.
6. Connect the negative battery cable.