For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel center molding.
2. Disconnect the cigar lighter and ashtray lamp electrical connector.
3. Remove the cigar lighter housing from the instrument panel.

### Installation Procedure

1. Install the cigar lighter housing to the instrument panel.
2. Install the cigar lighter in the cigar lighter housing.
3. Connect the cigar lighter and ashtray lamp electrical connector.
4. Install the instrument panel center molding.