For 1990-2009 cars

#### Tools Required

• | J 45059 Angle Meter or

• | KM-470-B Angular Torque Gage

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the timing belt. Refer to Timing Belt Replacement .
3. Remove the camshaft gears. Refer to Camshaft Gear Replacement .
4. Remove the timing belt automatic tensioner bolt.
5. Remove the timing belt automatic tensioner.
6. Remove the timing belt idler pulley bolt and nut.
7. Remove the timing belt idler pulleys.
8. Remove the engine mount retaining bolts.
9. Remove the engine mount.
10. Remove the crankshaft timing belt drive gear bolt.
11. Remove the crankshaft gear.
12. Remove the rear timing belt cover bolts.
13. Remove the rear timing belt cover.

### Installation Procedure

1. Install the rear timing belt cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear timing belt cover bolts.

Tighten
Tighten the rear timing belt cover bolts to 6 N·m (53 lb in).

3. Install the engine mount and the retaining bolts.

Tighten
Tighten the engine mount retaining bolts to 60 N·m (44 lb ft).

4. Install the timing belt idler pulleys.
5. Install the timing belt idler pulley bolt and nut.

Tighten

• | Tighten the timing belt idler pulley bolt to 25 N·m (18 lb ft).

• | Tighten the timing belt idler pulley nut to 25 N·m (18 lb ft).

6. Install the crankshaft timing belt drive gear and bolt.

Tighten
Tighten the crankshaft timing belt drive gear bolt to 145 N·m (107 lb ft) plus 30 degrees and plus 15 degrees using the J 45059 or the KM-470-B (1).

7. Install the timing belt automatic tensioner and bolt.

Tighten
Tighten the timing belt automatic tensioner bolt to 25 N·m (18 lb ft).

8. Install the camshaft gears. Refer to Camshaft Gear Replacement .
9. Install the timing belt and timing belt cover. Refer to Timing Belt Replacement .
10. Connect the negative battery cable.