For 1990-2009 cars

In addition to the steering function, the steering column provides safety and security.

The energy-absorbing column is designed to compress in a front-end collision to lessen the chance of driver injury.

The ignition switch and the lock are mounted on the column, allowing the ignition and steering operations to be locked to inhibit theft of the car.

The column levers trigger the turn signals, the headlight beams, and the windshield washer and wipers.

The tilt steering column uses telescopic function to allow the steering wheel to tilt up and down in and out. This enables the driver to adjust the steering wheel to a comfortable position.

The column may be disassembled and reassembled easily.

### Ignition Key Reminder

The ignition key reminder alerts the driver that the key is still in the ignition when the driver attempts to exit the vehicle.

An internal switch in the ignition lock cylinder supplies battery voltage to the reminder chime module when all of the following conditions are true:

• | The key is in the ignition switch.

• | The ignition is OFF.

• | The driver door is open.