For 1990-2009 cars

## Radio Antenna Module Replacement Sedan

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
3. Disconnect the electrical connector.
4. Remove the screws and the glass antenna module.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the glass antenna module with the screws.

Tighten
Tighten the glass antenna screws to 2 N·m (18 lb in).

2. Connect the electrical connectors.
3. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
4. Connect the negative battery cable.

## Radio Antenna Module Replacement Hatchback/Wagon

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the windshield garnish moulding. Refer to Windshield Pillar Garnish Molding Replacement .
3. Remove the sun visors. Refer to Sunshade Replacement .
4. Remove the headliner. Refer to Headlining Trim Panel Replacement .
5. Disconnect the antenna module electrical connector.
6. Remove the screws (1) and the antenna module.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the antenna module with the screws (1).

Tighten
Tighten the antenna module screws to 2 N·m (18 lb in).

2. Connect the antenna module electrical connector.
3. Install the headliner. Refer to Headlining Trim Panel Replacement .
4. Install the sun visors. Refer to Sunshade Replacement .
5. Install the windshield garnish moulding. Refer to Windshield Pillar Garnish Molding Replacement .
6. Connect the negative battery cable.