For 1990-2009 cars

## Starter Usage Gasoline Engines

Application | Description
--- | ---
Solenoid

- Hold-in Windings at 12 Volts

12-20 Amps

- Pull-in Windings at 12 Volts

60-90 Amps

Starter - 1.6L DOHC | 1.2 Kw

- Drive Pinion Speed

Min. 2,600 RPM

- No Load Test at 12 Volts

90 Amps Max.

Starter - 1.8L/2.0L DOHC | 1.4 Kw

- Drive Pinion Speed

Min. 2,550 RPM

- No Load Test at 12 Volts

85 Amps Max.