For 1990-2009 cars

### Removal Procedure

1. Disconnect negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement .
3. Slide the speed sensitive power steering (SSPS) control module off of the control module bracket.
4. Disconnect the electrical connector from the SSPS control module.

### Installation Procedure

1. Connect the electrical connector to the SSPS control module.
2. Slide the SSPS control module onto the control module bracket.
3. Install the glove box. Refer to Instrument Panel Storage Compartment Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.