For 1990-2009 cars

Table 1: | Hood Ajar Switch
Table 2: | Rear Compartment Lid Release Switch (Notchback)
Table 3: | Rear Compartment Lid Release Actuator (Notchback)
Table 4: | Rear Compartment Tamper Switch
Table 5: | Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/Alarm)
Table 6: | Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/o Alarm)
Table 7: | Security Indicator
Table 8: | Theft Deterrent Alarm

#### Hood Ajar Switch

Connector Part Information |

• | KET MG 610392

• | 2-Way F SDL Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 109 | Hood Ajar Switch Signal
2 | OG | 1240 | Battery Positive Voltage

#### Rear Compartment Lid Release Switch (Notchback)

Connector Part Information |

• | KET MG 651201

• | 2-Way F 090-II Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 253 | Trunk Release Relay Control
2 | OG | 640 | Battery Positive Voltage

#### Rear Compartment Lid Release Actuator (Notchback)

Connector Part Information |

• | KET MG 651032

• | 3-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 1250 | Ground
2 | BN | 253 | Trunk Ajar Switch Signal
3 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal

#### Rear Compartment Tamper Switch

Connector Part Information |

• | AMP 174463

• | 2-Way M 070 Series Multilock 2P (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal
2 | BK | 1250 | Ground
750

#### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/Alarm)

Connector Part Information |

• | KET MG 611336

• | 26-Way F PCB Connector (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE (North America) | 261 | Arm Alarm Signal
YE/D-GN
2 | BK | 350 | Ground
3 | -- | -- | Not Used
4 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal
5 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal
6 | -- | -- | Not Used
7 | PK/D-BU | 109 | Hood Ajar Switch Signal
8 | PU | 156 | Courtesy Lamp Control
9 | L-BU/BK (North America) | 195 | Door Unlock Control
L-BU
10 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
11 | YE | 356 | Driver Door Lock Relay Unlock Control
12 | L-GN | 1370 | Driver's Door Lock Switch
13 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
14 | -- | -- | Not Used
15 | PK | 639 | Ignition 1 Voltage
16 | -- | -- | Not Used
17 | L-GN | 483 | Serial Data
18 | L-GN/RD | 80 | Key In Ignition Switch Signal
19 | YE/D-GN | 749 | Security Indicator Control
20 | PU | 1371 | Door Lock Switch Signal
21-23 | -- | -- | Not Used
24 | BN | 253 | Trunk Release Relay Control (Notchback)
25 | OG | 340 | Battery Positive Voltage
26 | L-BU/BK | 14 | Left Turn Signal Lamps Supply Voltage
L-BU (North America)

#### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/o Alarm)

Connector Part Information |

• | 611336

• | 26-Way F PCB Connector (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 350 | Ground
3-7 | -- | -- | Not Used
8 | PU | 156 | Courtesy Lamp Control
9 | -- | -- | Not Used
10 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
11 | YE | 356 | Driver Door Lock Relay Unlock Control
12 | -- | -- | Not Used
13 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
14-16 | -- | -- | Not Used
17 | L-GN | 483 | Serial Data
18 | L-GN/RD | 80 | Key In Ignition Switch Signal
19-23 | -- | -- | Not Used
24 | BN | 253 | Trunk Release Relay Control (Notchback)
25 | OG | 340 | Battery Positive Voltage
26 | L-BU/BK | 14 | Left Turn Signal Lamps Supply Voltage
L-BU

#### Security Indicator

Connector Part Information |

• | KET MG 610070

• | 2-Way F 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | YE | 749 | Security Indicator Control

#### Theft Deterrent Alarm

Connector Part Information |

• | KUM PB 625-02027

• | 2-Way F NMWP 04F-B Ass'y (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | 261 | Arm Alarm Signal
2 | OG | 1240 | Battery Positive Voltage