For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement.
2. Remove the inside door handle. Refer to Door Inside Handle Replacement.
3. Disconnect the inside lock rods from the lock.

### Installation Procedure

1. Connect the inside lock rods to the lock.
2. Install the inside door handle. Refer to Door Inside Handle Replacement.
3. Install the door seal trim. Refer to Door Water Deflector Replacement.