For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the crankshaft position (CKP) sensor connector.
3. Remove the CKP sensor retaining bolt.
4. Gently rotate and remove the CKP sensor from the engine block.

### Installation Procedure

1. Insert the CKP sensor into the engine block.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CKP sensor retaining bolt.

Tighten
Tighten the CKP sensor retaining bolt to 6.5 N·m (57 lb in).

3. Connect the CKP sensor connector.
4. Connect the negative battery cable.