For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the left front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the bolts and the screws and the front wheel well splash shield.
4. Disconnect the electrical connector.
5. Disconnect the washer hose from the washer pump.
6. Remove the washer pump.

### Installation Procedure

1. Install the washer pump.
2. Connect the washer hose to the washer pump.
3. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the front wheel well splash shield with the bolts and screws.
5. Install the left front wheel. Refer to Tire and Wheel Removal and Installation .
6. Connect the negative battery cable.