For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Diagnostic System Check - Vehicle
2 | With a fused jumper wire, Connect terminals 4 and 5 of the fuel pump connector together. Did the Low Fuel Indicator turn on? | -- | Go to Step 7 | Go to Step 3
3 | Using a multimeter, test terminal 4 of the fuel pump connector for continuity to ground. Refer to Testing for Continuity . Is ground present? | -- | Go to Step 4 | Go to Step 5
4 | Using a multimeter, test for continuity between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Refer to Testing for Continuity . Is continuity present? | -- | Go to Step 8 | Go to Step 6
5 | Repair the open in ground circuit between terminal 4 of the fuel pump and ground 302. Refer to Wiring Repairs . Did you find and complete the repair? | -- | Go to Step 9 | --
6 | Repair the open in signal circuit between terminal 5 of the fuel pump connector and terminal B14 of the instrument cluster. Refer to Wiring Repairs . Did you find and complete the repair? | -- | Go to Step 9 | --
7 | Replace the fuel pump assembly. Refer to Fuel Pump Replacement for the 1.4L engine, Fuel Pump Replacement for the 1.8L engine, or Fuel Pump Replacement for the 2.0L engine. Did you complete the repair? | -- | Go to Step 9 | --
8 | Replace the low fuel indicator bulb. Refer to Instrument Cluster Bulb Replacement Did you complete the repair? | -- | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you find and complete the repair? | -- | System OK | Go to Step 2