For 1990-2009 cars

Important: Review the system description and operation in order to familiarize yourself with the system functions. Refer to Power Steering System Description and Operation .

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the power steering system.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

• | Inspect the power steering reservoir for the proper power steering fluid level and condition.

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom:

• | Variable Effort Steering Operating with Full Assist at all Times

• | Variable Effort Steering Operating with Decreased Assist at all Times

• | SSPS Warning Lamp Always On

• | SSPS Warning Lamp Inoperative

• | Power Steering System Test

• | Power Steering Fluid Leaks

• | Increase in Effort While Turning Steering Wheel

• | Poor Return of Steering Wheel

• | Steering Wheel Surges/Jerks While Turning

• | Steering Wheel Kickback

• | Steering Effort Hard in One or Both Directions

• | Too Much Play in Steering