For 1990-2009 cars

Table 1: | C101 - Floor Harness to Underhood Fuse Block
Table 2: | C102 - Floor Harness to Underhood Fuse Block
Table 3: | C103 - Engine Harness to Underhood Fuse Block
Table 4: | C104 - Front Harness to Underhood Fuse Block
Table 5: | C105 - Floor Harness to Underhood Fuse Block
Table 6: | C106 - Engine Harness to Underhood Fuse Block
Table 7: | C107 - ABS Harness to Underhood Fuse Block
Table 8: | C108 - Floor Harness to Engine Harness (1.4L, 1.6L)
Table 9: | C108 - Floor Harness to Engine Harness (1.8L, 2.0L)
Table 10: | C109 - Engine Harness to Front Harness
Table 11: | C110 - ABS Harness to Floor Harness
Table 12: | C111 - ABS Harness to Front Harness
Table 13: | C112 - Front Harness to Horn Jumper Harness
Table 14: | C113 - Floor Harness to Front Harness
Table 15: | C115 - Front Harness to Left Park/Turn Signal Lamp Jumper (North America)
Table 16: | C116 - Front Harness to Right Park/Turn Signal Lamp Jumper (North America)
Table 17: | C120 - Front Harness to Right Headlamp Jumper Harness (w/ Leveling) (Except North America)
Table 18: | C120 - Front Harness to Right Headlamp Jumper Harness (w/o Leveling) (North America)
Table 19: | C121 - Front Harness to Left Headlamp Jumper Harness (w/Leveling)
Table 20: | C121 - Front Harness to Left Headlamp Jumper Harness (w/o Leveling)
Table 21: | C135 - Engine Harness to Manifold Absolute Pressure (MAP) Sensor Jumper
Table 22: | C191 - ABS Harness to Left Front Wheel Speed Sensor Jumper
Table 23: | C192 - Front Harness to Right Front Wheel Speed Sensor Jumper
Table 24: | C201 - I/P Harness to I/P Fuse Block
Table 25: | C202 - I/P Harness to Floor Harness
Table 26: | C204 - Roof Harness to Floor Harness (w/ Rain Sensor)
Table 27: | C204 - Roof Harness to Floor Harness (w/o Rain Sensor)
Table 28: | C206 - I/P Harness to TCM Harness (Aisin)
Table 29: | C206 - I/P Harness to TCM Harness (ZF-4HP16)
Table 30: | C207 - SIR Harness to I/P Harness
Table 31: | C208 - I/P Harness to HVAC Harness (Auto A/C Only)
Table 32: | C209 - HVAC Harness to Auxiliary HVAC Harness (Auto A/C Only)
Table 33: | C301 - SIR Harness to Floor Harness (Except North America)
Table 34: | C301 - SIR to Floor Harness (North America)
Table 35: | C302 - I/P Harness to Console Harness
Table 36: | C351 - Floor Harness to Left Front Door Harness (LHD)
Table 37: | C351 - Floor Harness to Left Front Door Harness (RHD)
Table 38: | C361 - Floor Harness to Right Front Door Harness (LHD)
Table 39: | C361 - Floor Harness to Right Front Door Harness (RHD)
Table 40: | C371 - Floor Harness to Left Rear Door Harness
Table 41: | C381 - Floor Harness to Right Rear Door Harness
Table 42: | C391 - Rear ABS Harness to Left Rear Wheel Speed Sensor Jumper
Table 43: | C392 - Rear ABS Harness to Right Rear Wheel Speed Sensor Jumper
Table 44: | C401 - Trunk Harness to Floor Harness (Hatchback)
Table 45: | C401 - Trunk Harness to Floor Harness (Notchback)
Table 46: | C401 - Trunk Harness to Floor Harness (Optional)
Table 47: | C401 - Trunk Harness to Floor Harness (Notchback) (Optional)
Table 48: | C402 - Trunk Lid Harness to Floor Harness (Notchback)
Table 49: | C403 - Liftgate Jumper Harness to Floor Harness (Notchback)
Table 50: | C403 - Liftgate Jumper Harness to Floor Harness (Hatchback)
Table 51: | C404 - Liftgate Jumper Harness to Floor Harness (Notchback)
Table 52: | C404 - Liftgate Jumper Harness to Floor Harness (Hatchback)
Table 53: | C405 - Liftgate Jumper Harness to Liftgate Harness (Hatchback)
Table 54: | C405 - Liftgate Jumper Harness to Liftgate Harness (Notchback)
Table 55: | C406 - Liftgate Jumper Harness to Liftgate Harness (Hatchback)
Table 56: | C406 - Liftgate Jumper Harness to Liftgate Harness (Notchback)
Table 57: | C407 - Trunk Harness to Left Tail Lamp Jumper Harness (Hatchback)
Table 58: | C408 - Trunk Harness to Right Tail Lamp Jumper Harness (Hatchback)
Table 59: | C417 - Trunk Harness to Left Side Marker Lamp Jumper Harness
Table 60: | C418 - Trunk Harness to Right Side Marker Lamp Jumper Harness
Table 61: | C420 - Tailgate Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Hatchback)
Table 62: | C420 - Tailgate Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Notchback)
Table 63: | C421 - Tailgate Harness to Left Backup Lamp/Tail Lamp Jumper Harness (Notchback)
Table 64: | C421 - Tailgate Harness to Left Backup Lamp and Tail Lamp Jumper Harness (Hatchback)
Table 65: | C422 Tailgate Harness to License Lamps Jumper Harness (Hatchback)
Table 66: | C422 Tailgate Harness to License Lamps Jumper Harness (Notchback)
Table 67: | C423 - Floor Harness to Left Backup Lamp/Tail Lamp Jumper Harness (Optional)
Table 68: | C424 - Floor Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Optional)
Table 69: | C425 - Floor Harness to Left Side Marker Lamp Jumper Harness (Optional)
Table 70: | C426 - Floor Harness to Right Side Marker Lamp Jumper Harness (Optional)

#### C101 - Floor Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 612102

• | 21-Way F Hybrid 1809 Housing (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/GN (Except North America) | 267 | Heated Mirror Coil Supply Voltage
OG
2 | -- | -- | Not Used
3 | GY | 120 | Fuel Pump Supply Voltage
4 | WH (Except North America) | 193 | Rear Defog Relay Control
WH/BK
5 | PU/WH | 709 | Left Park Lamp Supply Voltage
PU (Except North America)
6 | PU/WH | 709 | Left Park Lamp Supply Voltage (Notchback LHD)
PU | 709 | Left Park Lamp Supply Voltage (Notchback RHD) (Hatchback LHD)
7 | BN | 141 | Ignition 3 Voltage
8 | L-GN | 876 | Rough Road Signal w/ ABS
9 | OG | 140 | Battery Positive Voltage
10 | BN/BK | 309 | Right Park Lamp Supply Voltage
11 | BN/WH | 309 | Right Park Lamp Supply Voltage
BN/BK (Except North America)
12 | -- | -- | Not Used
13 | PK/BK | 1846 | Ignition 1 Voltage
PK/BK | 1846 | Ignition 1 Voltage
14 | WH/BK | 1798 | Headlamp Relay Control
GY/BK (North America)
15 | PU/WH (Except North America) | 709 | Left Park Lamp Supply Voltage
PU/BK | 709 | Left Park Lamp Supply Voltage (Hatchback LHD)
PU | 709 | Left Park Lamp Supply Voltage (Notchback RHD)
16 | -- | -- | Not Used
17 | BK | 28 | Horn Relay Control
18 | WH | 1080 | Park Lamp Relay Control
19 | YE/D-GN | 317 | Fog Lamp Relay Coil Supply Voltage
20 | PU | 12 | Headlamp Low Beam Supply Voltage (Except North America)
L-BU | 1346 | Headlamp Supply Voltage/ Headlamp Control
21 | -- | -- | Not Used

#### C102 - Floor Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 652719

• | 11-Way F (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 12 | Headlamp Low Beam Supply Voltage
2 | L-GN | 11 | Headlamp High Beam Supply Voltage
3 | OG/BK | 1340 | Battery Positive Voltage
4 | PU | 293 | Rear Defog Element Supply Voltage
5 | RD | 581 | Power Window Supply Voltage - Driver Door
6 | OG/BK | 540 | Battery Positive Voltage
7 | PK | 539 | Ignition 1 Voltage
8 | OG/BK | 640 | Battery Positive Voltage
OG (Except North America)
9 | OG/BK | 640 | Battery Positive Voltage
OG (Except North America)
10 | OG/BK (Except North America) | 640 | Battery Positive Voltage
OG
11 | OG | 580 | Power Window Supply Voltage

#### C103 - Engine Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 651056

• | 10-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
-- | -- | Not Used (HV 240)
2 | PK/BK | 1846 | Ignition 1 Voltage
-- | -- | Not Used (HV 240)
3-4 | -- | -- | Not Used
5 | PK/BK | 1846 | Ignition 1 Voltage
-- | -- | Not Used (HV 240)
6 | BK | 1846 | Ignition 1 Voltage
PK/BK | 1846 | Ignition 1 Voltage (Sirius D4)
7 | PK/BK | 1846 | Ignition 1 Voltage
8 | -- | -- | Not Used
PK | 139 | Ignition 1 Voltage (Except North America) (Sirius D4)
9 | PK | 139 | Ignition 1 Voltage
PK | 139 | Ignition 1 Voltage
10 | PK | 139 | Ignition 1 Voltage
PK | 139 | Ignition 1 Voltage

#### C104 - Front Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 652503

• | 24-Way F Hybrid Connector (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage (Notchback) (Except North America)
2 | BN/WH | 309 | Right Park Lamp Supply Voltage (North America)
3 | PU | 34 | Fog Lamp Supply Voltage (w/Front Fog Lamp)
4 | BN | 990 | Power Steering Pressure Switch Signal (Except North America)
5 | D-GN | 59 | A/C Compressor Clutch Coil Supply Voltage (w/Air Conditioning)
6-7 | -- | -- | Not Used
8 | PU | 34 | Fog Lamp Supply Voltage (w/Front Fog Lamps)
9 | OG | 1240 | Battery Positive Voltage
OG | 1240 | Battery Positive Voltage
10 | -- | -- | Not Used
11 | YE | 712 | Left Headlamp Low Beam Supply Voltage
12 | BK | 50 | Ground
13-14 | -- | -- | Not Used
15 | L-BU | 409 | Cooling Fan Motor Supply Voltage
16 | PU | 312 | Right Headlamp Low Beam Supply Voltage
PU/WH (Except North America)
17 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
18 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
19 | PU | 709 | Left Park Lamp Supply Voltage (North America)
20 | PU | 709 | Left Park Lamp Supply Voltage (Notchback) (Except North America)
21 | PU | 532 | Cooling Fan Motor Supply Voltage
22 | PU | 532 | Cooling Fan Motor Supply Voltage
23 | D-GN | 29 | Horn Control
24 | -- | -- | Not Used

#### C105 - Floor Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 651926

• | 4-Way F 312-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD | 742 | Battery Positive Voltage
2 | RD/D-BU | 142 | Battery Positive Voltage
3 | RD/D-GN | 1642 | Battery Positive Voltage
4 | RD/WH | 642 | Battery Positive Voltage

#### C106 - Engine Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 651080

• | 20-Way F 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/D-BU | 539 | Ignition 1 Voltage
OG | 440 | Battery Voltage (Sirius D4)
2 | PK | 739 | Ignition 1 Voltage
3 | GY | 120 | Fuel Pump Supply Voltage
GY | 120 | Fuel Pump Supply Voltage
4 | D-GN/WH | 335 | Low Speed Cooling Fan Relay Control
D-GN (Except North America) | Low Speed Cooling Fan Relay Control
5 | D-BU | 473 | High Speed Cooling Fan Relay Control
D-BU | 473 | High Speed Cooling Fan Relay Control
6 | -- | -- | Not Used
7 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage
PU/WH | A/C Compressor Clutch Coil Supply Voltage (Sirius D4)
8 | OG | 440 | Battery Positive Voltage
9 | OG | 440 | Battery Positive Voltage
-- | -- | Not Used (Sirius D4)
10 | L-GN | 465 | Fuel Pump Relay Control
D-GN/WH | Fuel Pump Relay Control (Sirius D4)
11 | -- | -- | Not Used
12 | PK/D-BU | 539 | Ignition 1 Voltage
PK/D-BU | 539 | Ignition 1 Voltage
PK | 539 | Ignition 1 Voltage (Sirius D4)
13 | PK/D-BU | 539 | Ignition 1 Voltage
14 | PK/D-BU | 539 | Ignition 1 Voltage (Except North America)
15 | D-BU | 876 | Serial Data (w/ABS)
16 | -- | -- | Not Used
17 | BK | 250 | Ground
D-BU/WH | 471 | Main Relay Control (Sirius D4)
18 | -- | -- | Not Used
BN | 990 | Power Steering Pressure Switch Signal (Sirius D4)
19 | PK | 139 | Ignition 1 Voltage (HV 240)
BK | 250 | Ground (MR 140)
PK/D-BU | 539 | Ignition 1 Voltage (Sirius D4)
20 | -- | -- | Not Used

#### C107 - ABS Harness to Underhood Fuse Block

Connector Part Information |

• | KET MG 652500

• | 2-Way F 312-II Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD | 42 | Battery Positive Voltage
2 | RD | 42 | Battery Positive Voltage

#### C108 - Floor Harness to Engine Harness (1.4L, 1.6L)

Connector Part Information |

• | 96482026

• | 24-Way F (BK)

Connector Part Information

• | 96482027

• | 24-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1-A3 | -- | -- | Not Used | A1-A3 | -- | -- | Not Used
A4 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal | A4 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
A5 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control | A5 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
B1 | PU/BK | 632 | Low Reference | B1 | GY | 605 | Low Reference
B2 | D-GN/WH | 817 | Vehicle Speed Signal | B2 | D-GN/WH | 817 | Vehicle Speed Signal (w/ Manual Transmission)
B3 | D-GN/D-BU | 762 | A/C Request Signal | B3 | D-GN/WH | 762 | A/C Request Signal (w/ A/C)
B4 | WH/BK | 30 | Fuel Level Sensor Signal | B4 | WH | 30 | Fuel Level Sensor Signal
WH
C1 | D-GN | 890 | Fuel Tank Pressure Sensor Signal (North America) | C1 | YE/D-GN | 890 | Fuel Tank Pressure Sensor Signal (North America)
C2 | BN | 2000 | Serial Data | C2 | BN | 2000 | Serial Data
C3 | BN | 25 | Charge Indicator Control | C3 | BU | 25 | Charge Indicator Control
C4 | WH | 121 | Engine Speed Signal | C4 | WH | 121 | Engine Speed Signal
E1 | PU | 1807 | CAN Serial Data High | E1 | PU | 1807 | CAN Serial Data High (w/Automatic Transmission)
E2 | YE/RD | 710 | CAN Serial Data Low | E2 | YE | 710 | CAN Serial Data Low (w/Automatic Transmission)
E3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control (North America) | E3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
E4 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America) | E4 | L-BU/BK | 1986 | EVAP Canister Vent Solenoid Control (North America)
E5 | D-BU | 1936 | Fuel Level Sensor Signal | E5 | BU | 1936 | Fuel Level Sensor Signal
F1 | BN/BK | 231 | Engine Oil Pressure Switch Signal | F1 | BN/BK | 231 | Engine Oil Pressure Switch Signal
F2 | YE | 5 | Crank Voltage | F2 | YE | 5 | Crank Voltage
F3 | PK | 839 | Ignition 1 Voltage | F3 | PK | 839 | Ignition 1 Voltage (w/Manual Transmission)
F4 | L-GN | 24 | Backup Lamp Supply Signal | F4 | L-GN | 24 | Backup Lamp Supply Signal (w/Manual Transmission)
F5 | GY | 473 | High Speed Cooling Fan Relay Control | F5 | D-BU | 473 | High Speed Cooling Fan Relay Control
F6 | -- | -- | Not Used | F6 | -- | -- | Not Used

#### C108 - Floor Harness to Engine Harness (1.8L, 2.0L)

Connector Part Information |

• | 96482026

• | 24-Way F (BK)

Connector Part Information

• | 96482027

• | 24-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference (North America) | A1 | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference (North America)
A2 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal (North America) | A2 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal (North America)
A3 | GY | 605 | 5-Volt Reference (North America) | A3 | GY | 605 | 5-Volt Reference (North America)
A4 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal | A4 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
A5 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control | A5 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
B1 | PU/BK | 632 | Low Reference | B1 | PU/WH | 632 | Low Reference
B2 | D-GN/WH | 817 | Vehicle Speed Signal (w/ Manual Transmission) | B2 | D-GN/WH | 817 | Vehicle Speed Signal (w/ Manual Transmission)
B3 | D-GN/D-BU | 762 | A/C Request Signal (Except North America) | B3 | D-GN/WH | 762 | A/C Request Signal (Except North America)
D-GN | 762 | A/C Request Signal | D-GN | 762 | A/C Request Signal
B4 | WH/BK | 30 | Fuel Level Sensor Signal | B4 | WH | 30 | Fuel Level Sensor Signal
WH (Except North America)
C1 | D-GN | 890 | Fuel Tank Pressure Sensor Signal (North America) | C1 | YE/D-GN | 890 | Fuel Tank Pressure Sensor Signal (North America)
C2 | BN | 2000 | Serial Data | C2 | PU | 2000 | Serial Data
C3 | BN | 25 | Charge Indicator Control | C3 | BN | 25 | Charge Indicator Control
C4 | WH | 121 | Engine Speed Signal | C4 | GY | 121 | Engine Speed Signal
E1 | PU | 1807 | CAN Serial Data High | E1 | PU | 1807 | CAN Serial Data High (w/Automatic Transmission)
E2 | YE/BN | 710 | CAN Serial Data Low | E2 | YE | 710 | CAN Serial Data Low (w/Automatic Transmission)
E3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control (North America) | E3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
E4 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America) | E4 | L-BU/BK | 1986 | EVAP Canister Vent Solenoid Control (North America)
E5 | D-BU | 1936 | Fuel Level Sensor Signal | E5 | GY | 1936 | Fuel Level Sensor Signal
F1 | BN/BK | 231 | Engine Oil Pressure Switch Signal | F1 | BN/BK | 231 | Engine Oil Pressure Switch Signal
F2 | YE | 5 | Crank Voltage | F2 | YE | 5 | Crank Voltage
F3 | PK | 839 | Ignition 1 Voltage | F3 | PK | 839 | Ignition 1 Voltage (w/Manual Transmission)
F4 | L-GN | 24 | Backup Lamp Supply Signal | F4 | L-GN | 24 | Backup Lamp Supply Signal (w/Manual Transmission)
F5 | GY | 473 | High Speed Cooling Fan Relay Control | F5 | D-BU | 473 | High Speed Cooling Fan Relay Control
F6 | -- | -- | Not Used | F6 | -- | -- | Not Used

#### C109 - Engine Harness to Front Harness

Connector Part Information |

• | KET MG 651038

• | 4-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641041

• | 4-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference | 1 | BN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
L-GN (Sirius D4) | L-GN (Sirius D4)
2 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal | 2 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
3 | BN/WH | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control | 3 | BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
BN/BK (Sirius D4)
4 | PK/BK | 1846 | Ignition 1 Voltage | 4 | PK/BK | 1846 | Ignition 1 Voltage

#### C110 - ABS Harness to Floor Harness

Connector Part Information |

• | AMP 966196-5

• | 12-Way F (BU)

Connector Part Information

• | AMP 936207-5

• | 12-Way M 090-II 12P Cap Ass'y (BU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-BU | 20 | Stop Lamp Switch Signal | 1 | L-BU | 20 | Stop Lamp Switch Signal
2 | D-BU | 774 | Serial Data | 2 | D-BU/WH | 774 | Serial Data
3 | BN | 882 | Right Rear Wheel Speed Sensor Signal | 3 | BN | 882 | Right Rear Wheel Speed Sensor Signal
4 | BK | 884 | Left Rear Wheel Speed Sensor Signal | 4 | BK | 884 | Left Rear Wheel Speed Sensor Signal
5 | RD | 885 | Left Rear Wheel Speed Sensor Return | 5 | D-BU | 885 | Left Rear Wheel Speed Sensor Return
6 | BN | 739 | Ignition 1 Voltage | 6 | BN | 739 | Ignition 1 Voltage
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | L-GN/BK | 867 | ABS Indicator Failure Control | 8 | L-GN | 867 | ABS Indicator Failure Control
9 | L-GN | 876 | Rough Road Signal (Except North America) | 9 | WH | 876 | Rough Road Signal (Except North America)
WH/YE | 866 | Rough Road Signal | L-GN | 866 | Rough Road Signal
10 | WH | 883 | Right Rear Wheel Speed Sensor Return | 10 | WH | 883 | Right Rear Wheel Speed Sensor Return
11 | D-GN | 905 | Serial Data | 11 | D-GN | 905 | Serial Data
12 | PU/WH | 33 | Brake Warning Indicator Control | 12 | PU/WH | 33 | Brake Warning Indicator Control

#### C111 - ABS Harness to Front Harness

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322-5

• | 2-Way M SWP Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 833 | Front Right Wheel Speed Sensor Return | 1 | YE | 833 | Front Right Wheel Speed Sensor Return
2 | GY | 872 | Front Right Wheel Speed Sensor Signal | 2 | PU | 872 | Front Right Wheel Speed Sensor Signal

#### C112 - Front Harness to Horn Jumper Harness

Connector Part Information |

• | KET MG 641156

• | 2-Way F Econoseal J Mark II + Connector Plug Housing (BK)

Connector Part Information

• | AMP 6181-0080

• | 2-Way M Econoseal J-Mark II + Connector Cap Housing (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 50 | Ground | 1 | BK | 150 | Ground
2 | D-GN | 29 | Horn Control | 2 | BK/WH | 29 | Horn Control

#### C113 - Floor Harness to Front Harness

Connector Part Information |

• | AMP 368047-1

• | 16-Way F Econoseal J-Mark II + 16P Plug Assembly (BK)

Connector Part Information

• | AMP 368050-1

• | 16-Way M Econoseal J-MARK II + Connector 16Pos. CAP Housing (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 141 | Ignition 1 Voltage (Except North America) | 1 | PK | 741 | Ignition 1 Voltage (Except North America)
BN/BK | 2105 | Inflatable Restraint Front End Sensor - Left Voltage (North America) | BN/BK | 2105 | Inflatable Restraint Front End Discriminating Sensor - Left Voltage (North America)
2 | YE | 261 | Arm Alarm Signal | 2 | YE | 261 | Arm Alarm Signal
3 | PK/D-BU | 109 | Hood Ajar Switch Signal | 3 | PK/BK | 109 | Hood Ajar Switch Signal
4 | YE/D-BU | 61 | Low Reference (w/Auto A/C) | 4 | YE | 61 | Low Reference (w/Auto A/C)
5 | BN | 247 | Medium Blower Motor Control (Except North America) | 5 | BN | 247 | Medium Blower Motor Control (Except North America)
BN/WH
L-GN/RD | 2106 | Front End Sensor - Left Signal (North America) | L-GN/RD | 2106 | Inflatable Restraint Front End Discriminating Sensor - Left (North America)
6 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 6 | L-BU | 15 | Right Turn Signal Lamp Supply Voltage
7 | L-BU (Except North America) | 14 | Left Turn Signal Lamp Supply Voltage | 7 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
L-BU/BK
8 | L-GN/BK | 735 | Ambient Air Temperature Sensor (w/Auto A/C) | 8 | L-GN/BK | 735 | Ambient Air Temperature Sensor (w/Auto A/C)
9 | PU | 1703 | Variable Effort Steering Actuator Supply Voltage (w/Variable Effort Steering) | 9 | L-GN | 1703 | Variable Effort Steering Actuator Supply Voltage (w/Variable Effort Steering)
10 | GY | 473 | High Speed Cooling Fan Relay Control | 10 | GY | 473 | High Speed Cooling Fan Relay Control
11 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (w/Headlamp Leveling) | 11 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (w/Headlamp Leveling)
12 | RD | 228 | Windshield Washer Pump Control (Notchback) | 12 | RD | 228 | Windshield Washer Pump Control (Notchback)
13 | L-BU | 1738 | Variable Effort Steering Actuator Control (w/Variable Effort Steering) | 13 | BN/BK | 1738 | Variable Effort Steering Actuator Control (w/Variable Effort Steering)
14 | D-GN/WH | 2104 | Inflatable Restraint Front End Sensor - Right Signal (North America) | 14 | D-GN/WH | 2104 | Inflatable Restraint Front End Sensor - Right Signal (North America)
15 | PU | 2103 | Inflatable Restraint Front End Sensor - Right Voltage (North America) | 15 | PU | 2103 | Inflatable Restraint Front End Discriminating Sensor - Right (North America)
16 | PK/BK | 1846 | Ignition 1 Voltage | 16 | PK/BK | 1846 | Ignition 1 Voltage

#### C115 - Front Harness to Left Park/Turn Signal Lamp Jumper (North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640329

• | 3-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 50 | Ground | 2 | BK | 50 | Ground
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

#### C116 - Front Harness to Right Park/Turn Signal Lamp Jumper (North America)

Connector Part Information |

• | KET MG 610327

• | 3-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640329

• | 3-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | PU | 309 | Right Park Lamp Supply Voltage
2 | BK | 150 | Ground | 2 | BK | 150 | Ground
3 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage | 3 | PU | 15 | Right Turn Signal Lamps Supply Voltage

#### C120 - Front Harness to Right Headlamp Jumper Harness (w/ Leveling) (Except North America)

Connector Part Information |

• | KUM PB 625-06027

• | 6-Way F NMWP 06F-B Assembly (BK)

Connector Part Information

• | KUM PB 621-06020

• | 6-Way M NMWP 06M-B (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 150 | Ground | 1 | BK | 50 | Ground
2 | BN/WH | 309 | Right Park Lamp Supply Voltage | 2 | D-BU | 709 | Right Park Lamp Supply Voltage
3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage | 3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage
4 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | 4 | RD | 711 | Right Headlamp High Beam Supply Voltage
5 | PU/WH | 312 | Right Headlamp Low Beam Supply Voltage | 5 | L-GN | 712 | Right Headlamp Low Beam Supply Voltage
6 | BK | 150 | Ground | 6 | BK/WH | 50 | Ground

#### C120 - Front Harness to Right Headlamp Jumper Harness (w/o Leveling) (North America)

Connector Part Information |

• | KUM PB 625-04127

• | 4-Way F KNMWP 04F-GY Assembly (BK)

Connector Part Information

• | KUM PB 621-04120

• | 4-Way M Connector NMWP 04M-B (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 312 | Right Headlamp Low Beam Supply Voltage | 1 | L-GN | 312 | Right Headlamp Low Beam Supply Voltage
2 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | 2 | RD | 311 | Right Headlamp High Beam Supply Voltage
3 | BK | 150 | Ground | 3 | BK/WH | 150 | Ground
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### C121 - Front Harness to Left Headlamp Jumper Harness (w/Leveling)

Connector Part Information |

• | KUM PB 625-06027

• | 6-Way F NMWP 06F-B Assembly (BK)

Connector Part Information

• | KUM PB 621-06020

• | 6-Way M NMWP 06M-B (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 50 | Ground | 1 | BK | 50 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage | 2 | D-BU | 709 | Left Park Lamp Supply Voltage
3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage | 3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage
4 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | 4 | RD | 711 | Left Headlamp High Beam Supply Voltage
5 | YE | 712 | Left Headlamp Low Beam Supply Voltage | 5 | L-GN | 712 | Left Headlamp Low Beam Supply Voltage
6 | BK | 50 | Ground | 6 | BK/WH | 50 | Ground

#### C121 - Front Harness to Left Headlamp Jumper Harness (w/o Leveling)

Connector Part Information |

• | KUM PB 625-04127

• | 4-Way F KNMWP 04F-GY Assembly (BK)

Connector Part Information

• | KUM PB 621-04120

• | 4-Way M Connector NMWP04M-B (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 712 | Left Headlamp Low Beam Supply Voltage | 1 | L-GN | 712 | Left Headlamp Low Beam Supply Voltage
2 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | 2 | RD | 711 | Left Headlamp High Beam Supply Voltage
3 | BK | 50 | Ground | 3 | BK/WH | 50 | Ground
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### C135 - Engine Harness to Manifold Absolute Pressure (MAP) Sensor Jumper

Connector Part Information |

• | AMP 174357

• | 3-Way F Connector (BK)

Connector Part Information

• | AMP 174359

• | 3-Way M 070 Series Econoseal Mark-2 Cap 3P (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG/BK | 469 | Low Reference | 1 | OG/BK | 469 | Low Reference
2 | D-BU/WH | 432 | Manifold Absolute Pressure (MAP) Sensor Signal | 2 | L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
3 | L-BU/BK | 1688 | 5-Volt Reference | 3 | D-GN/BK | 1688 | 5-Volt Reference

#### C191 - ABS Harness to Left Front Wheel Speed Sensor Jumper

Connector Part Information |

• | Bosch 2264-420424 (F)

• | 2-Way F Connector (BK)

Connector Part Information

• | Bosch 2264-420424 (M)

• | 2-Way M Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 873 | Left Front Wheel Speed Sensor Signal | 1 | WH | 873 | Left Front Wheel Speed Sensor Signal
2 | L-BU | 830 | Left Front Wheel Speed Sensor Low Reference | 2 | BK | 830 | Left Front Wheel Speed Sensor Return

#### C192 - Front Harness to Right Front Wheel Speed Sensor Jumper

Connector Part Information |

• | Bosch 2264-420424 (F)

• | 2-Way F Connector (BK)

Connector Part Information

• | Bosch 2264-420424 (M)

• | 2-Way M Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 872 | Right Front Wheel Speed Sensor Signal | 1 | WH | 872 | Right Front Wheel Speed Sensor Return
2 | YE | 833 | Right Front Wheel Speed Sensor Low Reference | 2 | BK | 833 | Right Front Wheel Speed Sensor Signal

#### C201 - I/P Harness to I/P Fuse Block

Connector Part Information |

• | AMP 936195-1

• | 76-Way F Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 441 | Ignition 3 Voltage
2 | BK | 250 | Ground
3 | PK | 539 | Ignition 1 Voltage (Automatic Transmission)
PK | 539 | Ignition 1 Voltage (Automatic Transmission)
4 | BK | 250 | Ground
5 | PK | 339 | Ignition 1 Voltage
6 | PK | 239 | Ignition 1 Voltage (w/Manual A/C)
7 | PK | 239 | Ignition 1 Voltage (w/Manual A/C)
8 | PK | 239 | Ignition 1 Voltage (w/Variable Effort Steering)
9 | BK | 250 | Ground
10 | -- | -- | Not Used
11 | BN | 141 | Ignition 3 Voltage (Notchback Only w/Daytime Running Lamp (DRL)
12 | OG | 300 | Ignition 3 Voltage
13 | BN | 41 | Ignition 3 Voltage (w/Auto A/C)
14 | YE | 317 | Fog Lamp Relay Coil Supply Voltage (w/Rear Fog Lamps) (Except North America)
15 | YE | 317 | Fog Lamp Relay Coil Supply Voltage
16 | -- | -- | Not Used
17 | PK | 1139 | Ignition 1 Voltage (w/Air Bags)
18 | PK/OG | 239 | Ignition 1 Voltage (Except North America)
19 | PK | 239 | Ignition 1 Voltage (Key Interlock)
20 | PK | 239 | Ignition 1 Voltage (w/Alarm)
21 | PK | 239 | Ignition 1 Voltage (Notchback Only Daytime Running Lamp (DRL) Scandinavia)
22 | BK | 250 | Ground
23 | -- | -- | Not Used
24 | BN | 141 | Ignition 3 Voltage
25 | BN | 641 | Ignition 3 Voltage
BN | 641 | Ignition 3 Voltage
26 | YE | 317 | Fog Lamp Relay Coil Supply Voltage (w/Rear Fog Lamps)
27 | BN | 441 | Ignition 3 Voltage
28 | PK | 939 | Ignition 1 Voltage
29 | -- | -- | Not Used
30 | PK | 3 | Ignition 1 Voltage
PK | 3 | Ignition 1 Voltage
31 | PK | 239 | Ignition 1 Voltage
32 | PK | 239 | Ignition 1 Voltage (DAE)
33 | OG | 440 | Battery Positive Voltage
34 | OG | 1040 | Battery Positive Voltage
35 | BN | 41 | Ignition 3 Voltage (w/A/C)
36 | OG | 340 | Battery Positive Voltage (w/Alarm)
37 | OG | 1840 | Battery Positive Voltage
38 | YE | 317 | Fog Lamp Relay Coil Supply Voltage
39 | YE | 243 | Ignition 3 Voltage (Power Socket)
YE | 243 | Ignition 3 Voltage (Power Socket)
40 | BN | 441 | Ignition 3 Voltage
41 | OG | 140 | Battery Positive Voltage (w/Daytime Running Lamp (DRL)
42 | OG | 140 | Battery Positive Voltage
OG | 140 | Battery Positive Voltage
43 | PK | 739 | Ignition 1 Voltage (Notchback w/Cruise Control)
PK | 739 | Ignition 1 Voltage (Notchback w/Cruise Control)
BN | 739 | Ignition 1 Voltage (w/ABS)
44 | PK | 639 | Ignition 1 Voltage
45 | BK | 250 | Ground (Except North America)
46 | BK | 250 | Ground
47 | RD | 142 | Charge Indicator Control
48 | -- | -- | Not Used
49 | L-BU | 20 | Stop Lamp Switch Signal/Stop Lamp Supply Voltage
50 | L-BU | 20 | Stop Lamp Switch Signal/Stop Lamp Supply Voltage (w/Automatic Transmission)
51 | YE | 43 | Accessory Voltage
52 | YE | 43 | Accessory Voltage (w/Key Interlock)
53 | YE | 143 | Accessory Voltage
54 | PK | 639 | Ignition 1 Voltage (w/Immobilizer)
55 | PU/WH | 33 | Brake Warning Indicator Control
PU/WH | 33 | Brake Warning Indicator Control
56 | BK | 250 | Ground
57 | BK | 250 | Ground (Except North America)
58 | BK | 250 | Ground
59 | -- | -- | Not Used
60 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
61 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
62 | YE | 43 | Accessory Voltage (w/Key Interlock)
63 | YE | 43 | Accessory Voltage
64 | BN | 4 | Accessory Voltage
65 | OG | 140 | Battery Positive Voltage (w/Daytime Running Lamp (DRL) Scandinavian)
66 | PK | 839 | Ignition 1 Voltage (w/Automatic Transmission)
67 | PK | 839 | Ignition 1 Voltage
68 | PU/WH | 33 | Brake Warning Indicator Lamp
69 | BK | 250 | Ground (w/Dimming)
70 | BK | 250 | Ground
71 | -- | -- | Not Used
72 | OG | 1540 | Battery Positive Voltage
73 | OG | 1140 | Battery Positive Voltage
74 | OG | 40 | Battery Positive Voltage
75 | OG | 240 | Battery Positive Voltage (w/Immobilizer)
76 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C202 - I/P Harness to Floor Harness

Connector Part Information |

• | 96457410

• | 89-Way F Connector (WH)

Connector Part Information

• | 96457409

• | 89-Way M Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 247 | High Speed Blower Relay Control (w/Auto A/C) | 1 | BN | 247 | High Speed Blower Relay Control (w/Auto A/C)
BN/WH (Except North America)
2 | WH | 193 | Rear Defog Relay Control | 2 | WH | 193 | Rear Defog Relay Control
WH/BK (Except North America)
3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (w/Headlamp Leveling) | 3 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage
4 | GY | 161 | Antenna Module Signal | 4 | GY | 161 | Antenna Module Signal
5 | BN | 141 | Ignition 3 Voltage | 5 | BN | 141 | Ignition 3 Voltage
6 | BN | 641 | Ignition 3 Voltage | 6 | BN (Except North America) | 641 | Ignition 3 Voltage
BN/WH
7 | BK/WH | 238 | Seat Belt Switch Left | 7 | BK/WH | 238 | Seat Belt Switch Left
8 | YE | 112 | Windshield Wiper Switch Signal 1 | 8 | YE | 112 | Windshield Wiper Switch Signal 1
9 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal | 9 | D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
10 | PU/WH | 33 | Brake Warning Indicator Control | 10 | PU/WH | 33 | Brake Warning Indicator Control
RD | 122 | Rear Fog Lamp Supply Voltage (Except North America) | RD | 122 | Rear Fog Lamp Supply Voltage (Except North America)
11 | L-BU | 20 | Stop Lamp Switch Signal | 11 | L-BU | 20 | Stop Lamp Switch Signal
12 | L-GN | 483 | Serial Data (w/Alarm) | 12 | L-GN | 483 | Serial Data (w/Alarm)
PK/BK | 1303 | Door Switch Signal (Except North America) | PK/BK | 1303 | Door Switch Signal (Except North America)
13 | BN | 25 | Charge Indicator Signal | 13 | BN | 25 | Charge Indicator Signal
14 | YE | 317 | Front Fog Lamp Relay Coil Supply Voltage | 14 | YE/D-GN | 317 | Front Fog Lamp Relay Coil Supply Voltage
15 | PU | 126 | Left Front Door Open Switch Signal | 15 | PU/WH | 126 | Left Front Door Open Switch Signal
16 | WH | 905 | Serial Data (w/ABS) | 16 | D-GN | 905 | Serial Data (w/ABS)
17 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 17 | L-BU/BK (Except North America) | 14 | Left Turn Signal Lamp Supply Voltage
L-BU
18 | OG | 340 | Battery Positive Voltage (w/Alarm) | 18 | OG | 340 | Battery Positive Voltage (w/Alarm)
19 | D-BU/WH | 774 | Serial Data (w/ABS) | 19 | D-BU/WH | 774 | Serial Data (w/ABS)
20 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 20 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
21 | PU | 2000 | Serial Data | 21 | BN | 2000 | Serial Data
22 | L-GN | 867 | ABS Indicator Failure Control (w/ABS) | 22 | L-GN/BK | 867 | ABS Indicator Failure Control 1 (w/ABS)
23 | L-BU | 97 | Windshield Wiper Switch Mist/OFF/Low Signal | 23 | BN | 96 | Windshield Wiper Switch Delay Signal
24 | L-BU | 263 | Tamper Switch Signal (Optional) | 24 | L-BU | 263 | Tamper Switch Signal (Optional)
25 | D-GN | 1659 | Microphone (-) (Optional) | 25 | WH | 1659 | Microphone (-) (Optional)
26 | YE | 356 | Door Lock (Optional) | 26 | YE | 356 | Door Lock (Optional)
27 | PK/BK | 109 | Alarm Signal (Optional) | 27 | PK/BK | 109 | Alarm Signal (Optional)
28 | WH | 1658 | Microphone (+) (Optional) | 28 | D-BU | 1658 | Microphone (+) (Optional)
29 | L-GN/WH | 355 | Door Unlock (Optional) | 29 | L-GN/WH | 355 | Door Unlock (Optional)
30 | WH | 156 | Courtesy Lamp Control | 30 | PU | 156 | Courtesy Lamp Control
31 | WH | 1080 | Park Lamp Relay Control (w/Lamp Driver Control Module) | 31 | WH | 1080 | Park Lamp Relay Control
32 | PU/WH | 231 | Oil Pressure Switch Signal | 32 | BN/BK | 231 | Oil Pressure Switch Signal
PU/BK (Except North America) | PU/WH (Except North America) | 231 | Oil Pressure Daytime Running Lamp (DRL) Input (Scandinavian)
33 | D-GN/WH | 762 | A/C Request Signal (w/A/C) | 33 | D-GN/D-BU | 762 | A/C Request Signal (w/A/C)
34 | L-GN | 11 | Headlamp High Beam Supply Voltage | 34 | L-GN | 11 | Headlamp High Beam Supply Voltage
35 | BK | 28 | Horn Relay Control | 35 | BK | 28 | Horn Relay Control
36 | D-BU | 744 | Trunk Open Signal | 36 | D-BU | 744 | Trunk Open Signal
L-BU | 195 | Door Lock (Except North America) | L-BU | 195 | Door Lock (Except North America)
PK/BK | 1303 | Door Switch Signal (Except North America) | PK/BK | 1303 | Door Switch Signal (Except North America)
37 | -- | -- | Not Used | 36-37 | -- | -- | Not Used
38 | YE | 749 | Security Indicator Control (w/Immobilizer) | 38 | YE/D-GN | 749 | Security Indicator Control (w/Immobilizer)
39 | BN/WH | 309 | Right Park Lamp Supply Voltage | 39 | BN/BK | 309 | Right Park Lamp Supply Voltage
40 | OG | 540 | Battery Positive Voltage | 40 | OG/BK | 540 | Battery Positive Voltage
41 | PU/WH | 33 | Brake Warning Indicator Control | 41 | PU/WH | 33 | Brake Warning Indicator Control
42 | PK | 839 | Ignition 1 Voltage | 42 | PK | 839 | Ignition 1 Voltage
43 | RD | 228 | Windshield Washer Pump Control | 43 | RD | 228 | Windshield Washer Pump Control
44 | PU | 12 | Headlamp Low Beam Supply Voltage | 44 | PU | 12 | Headlamp Low Beam Supply Voltage
45 | OG | 640 | Battery Positive Voltage | 45 | OG/BK | 640 | Battery Positive Voltage
OG | 640 | Battery Positive Voltage | OG/BK | 640 | Battery Positive Voltage
46 | BN | 641 | Ignition 3 Voltage | 46 | BN | 641 | Ignition 3 Voltage
BN/BK (Except North America)
47 | BN | 441 | Ignition 3 Voltage | 47 | RD/D-BU | 441 | Ignition 3 Voltage
48 | PK | 639 | Ignition 1 Voltage | 48 | PK | 639 | Ignition 3 Voltage
49 | L-GN | 80 | Key In Ignition Switch Signal (w/Alarm) | 49 | L-GN/RD | 80 | Key In Ignition Switch Signal (w/Alarm)
BN | 253 | Trunk Open (Except North America) | BN | 253 | Trunk Open (Except North America)
50 | YE | 243 | Accessory Voltage | 50 | YE | 243 | Accessory Voltage
51 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control | 51 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
52 | RD | 1642 | Battery Positive Voltage | 52 | RD/D-GN | 1642 | Battery Positive Voltage
53 | YE | 5 | Crank Voltage (Except North America) | 53 | YE | 5 | Crank Voltage (Except North America)
PU | 5 | Crank Voltage | 5 | Crank Voltage
54 | OG | 140 | Battery Positive Voltage | 54 | OG | 140 | Battery Positive Voltage
55 | RD | 742 | Battery Positive Voltage | 55 | RD | 742 | Battery Positive Voltage
56 | RD | 142 | Battery Positive Voltage | 56 | RD/D-BU | 142 | Battery Positive Voltage
57 | L-BU | 1346 | Headlamp Supply Voltage | 57 | L-BU | 1346 | Headlamp Supply Voltage
58 | PK | 539 | Ignition 1 Voltage | 58 | PK | 539 | Ignition 1 Voltage
59 | RD | 642 | Battery Positive Voltage | 59 | RD/WH | 642 | Battery Positive Voltage
60 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal (w/Auto A/C) | 60 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
61 | YE | 61 | Low Reference (w/Auto A/C) | 61 | YE/D-BU | 61 | Low Reference
62 | PK | 739 | Ignition 1 Voltage (w/ABS) | 62 | BN | 739 | Ignition 1 Voltage (w/ABS)
63 | D-GN/WH | 817 | Vehicle Speed Signal | 63 | D-GN/WH | 817 | Vehicle Speed Signal
64 | D-GN | 392 | Rear Window Washer Pump Control | 64 | D-GN | 392 | Rear Window Washer Pump Control (Hatchback Only)
65 | D-GN | 95 | Windshield Washer Switch Signal | 65 | D-GN | 95 | Windshield Washer Switch Signal
66 | GY | 121 | Engine Speed Signal | 66 | WH | 121 | Engine Speed Signal
67 | PU | 92 | Windshield Wiper Motor High Speed | 67 | PU | 92 | Windshield Wiper Motor High Speed
68 | PU | 201 | Left Front Speaker Output (+) | 68 | PU | 201 | Left Front Speaker Output (+)
69 | YE | 710 | CAN Serial Data Low (w/Automatic Transmission) | 69 | YE/BN | 710 | CAN Serial Data Low
70 | WH | 393 | Rear Window Wiper Motor Control | 70 | WH | 393 | Rear Window Wiper Motor Control (Hatchback Only)
71 | L-BU | 115 | Right Rear Speaker Output (-) | 71 | L-BU | 115 | Right Rear Speaker Output (-)
72 | PU | 1807 | CAN Serial Data High (w/Automatic Transmission) | 72 | PU | 1807 | CAN Serial Data High
73 | D-GN/WH | 900 | Key Cylinder Lamp Control (Notchback Only) | 73 | D-GN/WH | 900 | Key Cylinder Lamp Control
74 | L-GN | 200 | Right Front Speaker Output (+) | 74 | L-GN | 200 | Right Front Speaker Output (+)
75 | L-GN | 24 | Backup Lamp Supply Voltage (w/Automatic Transmission) | 75 | L-GN | 24 | Backup Lamp Supply Voltage
76 | RD | 709 | Left Park Lamp Supply Voltage (w/Alarm) | 76 | PU/WH | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage (Notchback RHD)
77 | GY | 118 | Left Front Speaker Output (-) | 77 | GY/WH | 118 | Left Front Speaker Output (-)
78 | GY/BK | 1798 | Headlamp Relay Control | 78 | GY/BK | 1798 | Headlamp Relay Control
79 | -- | -- | Not Used | 79 | -- | -- | Not Used
BN/WH | 1201 | Left Front Speaker Output (-) (Except Notchback RHD) | BN/WH | 1201 | Left Front Speaker Output (-) (Except Notchback RHD)
GY | 1118 | GY | 1118
80 | YE | 116 | Left Rear Speaker Output (-) | 80 | YE | 116 | Left Rear Speaker Output (-)
81 | PU | 172 | Low Fuel Indicator Control | 81 | PU | 172 | Low Fuel Indicator Control
82 | -- | -- | Not Used | 82 | -- | -- | Not Used
GY | 1118 | Left Front Speaker Output (+) (Except Notchback RHD) | GY | 1118 | Left Front Speaker Output (+) (Except Notchback RHD)
BN/WH | 1201 | BN/WH | 1201
83 | BN | 199 | Left Rear Speaker Output (+) | 83 | BN | 199 | Left Rear Speaker Output (+)
84 | -- | -- | Not Used | 84 | -- | -- | Not Used
YE | 261 | Alarm Signal (Except North America) | YE | 261 | Alarm Signal (Except North America)
85 | WH | 30 | Fuel Level Sensor Signal | 85 | WH/BK | 30 | Fuel Level Sensor Signal
86 | D-BU | 46 | Right Rear Speaker Output (+) | 86 | D-BU/WH | 46 | Right Rear Speaker Output (+)
87 | L-BU | 1738 | Variable Effort Steering Actuator Supply Voltage (w/Variable Effort Steering) | 87 | L-BU | 1738 | Variable Effort Steering Actuator Supply Voltage
88 | PU | 1703 | Variable Effort Steering Actuator Control | 88 | PU | 1703 | Variable Effort Steering Actuator Control
89 | D-GN | 117 | Right Front Speaker Output (-) | 89 | D-GN | 117 | Right Front Speaker Output (-)

#### C204 - Roof Harness to Floor Harness (w/ Rain Sensor)

Connector Part Information |

• | AMP 936199-1

• | 14-Way F Connector (WH)

Connector Part Information

• | AMP 936209-1

• | 14-Way M Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-GN | 227 | Windshield Washer Pump Ground | 1 | L-GN | 227 | Windshield Washer Pump Ground
2 | D-GN | 2228 | Wiper Motor Signal | 2 | D-GN | 2228 | Wiper Motor Signal
3 | D-BU | 1112 | Wiper Motor Signal | 3 | D-BU | 1112 | Wiper Motor Signal
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
WH | 1659 | Microphone (-) (Optional) | WH | 1659 | Microphone (-) (Optional)
5 | GY | 161 | Antenna Enable Signal | 5 | GY | 161 | Antenna Motor Up
6 | PU | 156 | Courtesy Lamp Control | 6 | PU | 156 | Courtesy Lamp Control
7 | PK | 839 | Ignition 1 Voltage | 7 | PK | 839 | Ignition 1 Voltage
8 | YE | 112 | Windshield Wiper Switch Signal 1 | 8 | YE | 112 | Windshield Wiper Switch Signal
9 | RD | 228 | Windshield Washer Pump Control | 9 | RD | 228 | Windshield Washer Pump Control
10 | PK | 639 | Ignition 1 Voltage | 10 | RD/D-BU | 441 | Ignition 1 Voltage (Notchback RHD)
PK | 639 | Ignition 1 Voltage (Notchback LHD)
11 | D-GN/WH | 900 | Key Cylinder Lamp Control | 11 | D-GN/WH | 900 | Key Cylinder Lamp Control
12 | OG | 640 | Battery Positive Voltage | 12 | OG/BK | 640 | Battery Positive Voltage
13 | BN | 641 | Ignition 3 Voltage | 13 | BN/WH | 641 | Ignition 3 Voltage
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
PK/BK | 1303 | Door Switch Signal | PK/BK | 1303 | Door Switch Signal
D-BU | 1658 | Microphone (+) (Optional) | D-BU | 1658 | Microphone (+) (Optional)

#### C204 - Roof Harness to Floor Harness (w/o Rain Sensor)

Connector Part Information |

• | AMP 936233

• | 8-Way F 090III 8P PLUG Assembly (WH)

Connector Part Information

• | AMP 936242

• | 8-Way M 090III 8P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GY | 161 | Antenna Signal | 1 | GY | 161 | Antenna Motor Up (Hatchback Only)
2 | PU | 156 | Courtesy Lamp Control | 2 | PU | 156 | Courtesy Lamp Control
3 | PK | 839 | Ignition 1 Voltage | 3 | PK | 839 | Ignition 1 Voltage
4 | D-GN/WH | 900 | Key Cylinder Lamp Control | 4 | D-GN/WH | 900 | Key Cylinder Lamp Control
5 | OG | 640 | Battery Positive Voltage | 5 | OG | 640 | Battery Positive Voltage
OG/BK (Except North America)
6 | BN | 641 | Ignition 3 Voltage | 6 | BN/WH | 641 | Ignition 3 Voltage (Hatchback)
BN | 641 | Ignition 3 Voltage | BN | 641 | Ignition 3 Voltage (Notchback)
7 | D-BU | 1658 | Microphone (+) (Optional) | 7 | D-BU | 1658 | Microphone (+) (Optional)
8 | WH | 1659 | Microphone (-) (Optional) | 8 | WH | 1659 | Microphone (-) (Optional)
PK/BK | 1303 | Door Switch Signal (Except North America) | PK/BK | 1303 | Door Switch Signal (Except North America)

#### C206 - I/P Harness to TCM Harness (Aisin)

Connector Part Information |

• | KET MG 610837

• | 22-Way F Hybrid 2507 Housing (WH)

Connector Part Information

• | KET MG 620838

• | 22-Way M Hybrid 2507 Housing (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-GN/WH | 1135 | Transmission Hold Signal | 1 | D-GN/WH | 1135 | Transmission Hold Signal
2 | L-GN/BK | 3013 | Park/Neutral Position (PNP) Switch Drive Signal | 2 | WH | 2377 | Park/Neutral Position (PNP) Switch Drive Signal
3 | D-GN/WH | 817 | Vehicle Speed Signal | 3 | D-GN/WH | 817 | Vehicle Speed Signal
4 | YE | 710 | CAN Serial Data Low | 4 | YE | 710 | CAN Serial Data Low
5 | YE | 1481 | Hold Mode Indicator Control | 5 | YE | 1481 | Hold Mode Indicator Control
6 | L-GN/RD | 3012 | Park/Neutral Position (PNP) Switch Neutral Signal | 6 | YE | 2381 | Park/Neutral Position (PNP) Switch Neutral Signal
7 | BK | 250 | Ground | 7 | BK/WH | 51 | Ground
8 | OG/BK | 434 | Automatic Transmission Shift Lock Control | 8 | OG/BK | 434 | Automatic Transmission Shift Lock Control
9 | L-BU | 20 | Stop Lamp Supply Voltage/ Stop Lamp Switch Signal | 9 | L-BU | 20 | Stop Lamp Supply Voltage/ Stop Lamp Switch Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | L-GN/RD | 3011 | Park/Neutral Position (PNP) Switch Reverse Signal | 11 | D-GN/WH | 2383 | Park/Neutral Position (PNP) Switch Reverse Signal
12 | PK | 539 | Ignition 1 Voltage | 12 | PK | 839 | Ignition 1 Voltage
13-14 | -- | -- | Not Used | 13-14 | -- | -- | Not Used
15 | D-GN | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal | 15 | PK | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal
16 | D-BU/RD | 3010 | Park/Neutral Position (PNP) Switch Park Signal | 16 | D-GN | 2382 | Park/Neutral Position (PNP) Switch Park Signal
17 | L-GN | 24 | Backup Lamp Supply Voltage | 17 | D-GN/WH | 24 | Backup Lamp Supply Voltage
18 | OG | 440 | Battery Positive Voltage | 18 | OG | 440 | Battery Positive Voltage
19 | PU | 2000 | Keyword Serial Data | 19 | D-BU | 2000 | Keyword Serial Data
20 | PK | 839 | Ignition 1 Voltage | 20 | -- | -- | Not Used
21 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal | 21 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal
22 | PU | 1807 | CAN Serial Data High | 22 | PU | 1807 | CAN Serial Data High

#### C206 - I/P Harness to TCM Harness (ZF-4HP16)

Connector Part Information |

• | KET MG 610837

• | 22-Way F Hybrid 2507 Housing (WH)

Connector Part Information

• | KET MG 620838

• | 22-Way M Hybrid 2507 Housing (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-GN/WH | 1135 | Transmission Hold Signal | 1 | D-GN/WH | 1135 | Transmission Hold Signal
2 | L-GN/BK | 3013 | Park/Neutral Position (PNP) Switch L4 Signal | 2 | L-GN/BK | 3013 | Park/Neutral Position (PNP) Switch L4 Signal
3 | D-GN/WH | 817 | Vehicle Speed Signal | 3 | D-GN/WH | 817 | Vehicle Speed Signal
4 | YE | 710 | CAN Serial Data Low | 4 | YE | 710 | CAN Serial Data Low
5 | YE | 1481 | Hold Mode Indicator Control | 5 | YE | 1481 | Hold Mode Indicator Control
6 | L-GN/RD | 3012 | Park/Neutral Position (PNP) Switch L3 Signal | 6 | RD/ D-BU | 3012 | Park/Neutral Position (PNP) Switch L3 Signal
7 | BK | 250 | Ground | 7 | BK/WH | 251 | Ground
8 | OG/BK | 434 | Automatic Transmission Shift Lock Control | 8 | OG/BK | 434 | Automatic Transmission Shift Lock Control
9 | L-BU | 20 | Stop Lamp Supply Voltage/ Stop Lamp Switch Signal | 9 | L-BU | 20 | Stop Lamp Supply Voltage/ Stop Lamp Switch Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | L-GN/RD | 3011 | Park/Neutral Position (PNP) Switch L2 Signal | 11 | L-GN/RD | 3011 | Park/Neutral Position (PNP) Switch L2 Signal
12 | PK | 539 | Ignition 1 Voltage | 12 | PK | 439 | Ignition 1 Voltage
13-14 | -- | -- | Not Used | 13-14 | -- | -- | Not Used
15 | D-GN | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal (Except North America) | 15 | D-GN | 3017 | Transmission Mode Signal Power
16 | D-BU/RD | 3010 | Park/Neutral Position (PNP) Switch L1 Signal | 16 | D-BU/RD | 3010 | Park/Neutral Position (PNP) Switch L1 Signal
17 | L-GN | 24 | Backup Lamp Supply Voltage | 17 | L-GN | 24 | Backup Lamp Supply Voltage
18 | OG | 440 | Battery Positive Voltage | 18 | OG | 440 | Battery Positive Voltage
19 | PU | 2000 | Keyword Serial Data | 19 | BN | 2000 | Keyword Serial Data
20 | PK | 839 | Ignition 1 Voltage | 20 | PK | 839 | Ignition 1 Voltage
21 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal (Except North America) | 21 | -- | -- | Not Used
22 | PU | 1807 | CAN Serial Data High | 22 | PU | 1807 | CAN Serial Data High

#### C207 - SIR Harness to I/P Harness

Connector Part Information |

• | AMP 175658

• | 6-Way F 070 MLC W-W PLUG HSG 6P (WH)

Connector Part Information

• | AMP 175657

• | 6-Way M .070 SRS MLC 6POS (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 1139 | Ignition 1 Voltage | 1 | PK | 1139 | Ignition 1 Voltage
2 | BN/WH | 238 | Seat Belt Switch Left | 2 | BK/WH | 238 | Seat Belt Switch Left
3 | D-GN | 358 | Air Bag Indicator Control | 3 | BN | 358 | Air Bag Indicator Control
4 | L-BU | 327 | SIR Serial Data | 4 | L-BU | 327 | SIR Serial Data
5 | -- | -- | Not Used (RHD) | 5 | -- | -- | Not Used (RHD)
PK | 939 | Ignition 1 Voltage (LHD) | PK | 939 | Ignition 1 Voltage (LHD)
6 | D-GN/WH | 1358 | Air Bag Indicator Control (North America Only) | 6 | D-GN/WH | 1358 | Air Bag Indicator Control (North America Only)

#### C208 - I/P Harness to HVAC Harness (Auto A/C Only)

Connector Part Information |

• | AMP 85113-1

• | 15-Way F 070/250 Series Hybrid 15P Plug Housing (WH)

Connector Part Information

• | AMP 85114-1

• | 15-Way M .070/.250 Hybrid 15P CAP HSG (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 61 | Low Reference | 1 | YE | 61 | Low Reference
2 | D-GN/WH | 762 | A/C Request Signal | 2 | D-GN/WH | 762 | A/C Request Signal
3 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal | 3 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
4 | BN/WH | 309 | Right Park Lamp Supply Voltage | 4 | BN/WH | 309 | Right Park Lamp Supply Voltage
5 | D-GN/WH | 817 | Vehicle Speed Signal | 5 | D-GN/RD | 817 | Vehicle Speed Signal
6 | BN | 41 | Ignition 3 Voltage | 6 | BN | 41 | Ignition 3 Voltage
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | OG | 1140 | Battery Positive Voltage | 8 | OG | 1140 | Battery Positive Voltage
9 | L-GN/BK | 735 | Ambient Air Temperature Sensor | 9 | L-GN/BK | 735 | Ambient Air Temperature Sensor
10 | BN | 247 | High Speed Blower Relay Control | 10 | -- | -- | Not Used
11 | WH | 193 | Rear Defog Relay Control | 11 | WH | 193 | Rear Defog Relay Control
12 | PU | 65 | Blower Motor Feed | 12 | YE | 744 | Blower Motor Supply Voltage
13 | BK | 1050 | Ground | 13 | BK | 350 | Ground
14 | D-GN | 95 | Windshield Washer Switch Signal | 14 | D-GN | 95 | Windshield Washer Switch Signal
15 | -- | -- | Not Used | 15 | -- | -- | Not Used

#### C209 - HVAC Harness to Auxiliary HVAC Harness (Auto A/C Only)

Connector Part Information |

• | AMP 368511-1

• | 20-Way F 070 Multi Lock Connector (WH)

Connector Part Information

• | AMP 368510-1

• | 20-Way M 070 Multi Lock Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG | 1140 | Battery Positive Voltage | 1 | OG | 1140 | Battery Positive Voltage
2 | PK/WH | 1648 | Recirculation Door Control A | 2 | PK/WH | 1648 | Recirculation Door Control A
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | D-GN/BK | 1647 | Recirculation Door Control B | 4 | D-GN/BK | 1647 | Recirculation Door Control B
5 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal | 5 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
6 | D-BU/BK | 247 | High Speed Blower Relay Control | 6 | D-BU/BK | 247 | High Speed Blower Relay Control
7 | D-GN | 95 | Windshield Washer Switch Signal | 7 | D-GN | 95 | Windshield Washer Switch Signal
8 | D-GN/RD | 817 | Vehicle Speed Signal | 8 | D-GN/RD | 817 | Vehicle Speed Signal
9 | D-BU | 188 | Blower Motor Supply Voltage | 9 | D-BU | 188 | Blower Motor Supply Voltage
10 | WH | 193 | Rear Defog Relay Signal | 10 | WH | 193 | Rear Defog Relay Signal
11 | BN | 41 | Ignition 3 Voltage | 11 | BN | 41 | Ignition 3 Voltage
12 | BN/WH | 309 | Right Park Lamp Supply Voltage | 12 | BN/WH | 309 | Right Park Lamp Supply Voltage
13 | D-GN | 44 | Instrument Panel Lamps Dimming Control | 13 | D-GN | 44 | Instrument Panel Lamps Dimming Control
14 | BN/WH | 762 | A/C Request Signal | 14 | BN/WH | 762 | A/C Request Signal
15 | YE | 61 | Low Reference | 15 | YE | 61 | Low Reference
16-18 | -- | -- | Not Used | 16-18 | -- | -- | Not Used
19 | BK | 350 | Ground | 19 | BK | 350 | Ground
20 | GY/BK | 754 | Blower Motor Speed Control | 20 | GY/BK | 754 | Blower Motor Speed Control

#### C301 - SIR Harness to Floor Harness (Except North America)

Connector Part Information |

• | AMP 936233-1

• | 8-Way F 090III 8P PLUG Assembly (WH)

Connector Part Information

• | AMP 936242-1

• | 8-Way M 090III 8P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RD/YE | 753 | Side Impact Sensor - Driver Voltage | 1 | PK | 753 | Side Impact Sensor - Driver Voltage
2 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage | 2 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage
3 | PK | 1184 | Seat Belt Pretensioner - Driver Low Control | 3 | YE/D-BU | 1184 | Seat Belt Pretensioner - Driver Low Control
4 | BK | 754 | Side Impact Sensor - Driver Signal | 4 | BK/WH | 754 | Side Impact Sensor - Driver Signal
5 | BN/WH | 715 | Side Impact Sensor - Passenger Signal | 5 | BN/WH | 715 | Side Impact Sensor - Passenger Signal
6 | D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger Low Control | 6 | RD/BK | 1187 | Seat Belt Pretensioner - Passenger Low Control
7 | PK/BK | 1186 | Seat Belt Pretensioner - Passenger High Control | 7 | D-BU/WH | 1186 | Seat Belt Pretensioner - Passenger High Control
8 | D-BU | 1185 | Seat Belt Pretensioner - Driver High Control | 8 | PU | 1185 | Seat Belt Pretensioner - Driver High Control

#### C301 - SIR to Floor Harness (North America)

Connector Part Information |

• | AMP 936196-1

• | 12-Way F 090 III 12P Plug Assembly (WH)

Connector Part Information

• | AMP 936207-5

• | 12-Way M 090-II 12P Cap Assembly (BU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 2103 | Front End Sensor - Right - Voltage | 1 | PU | 2103 | Front End Sensor - Right - Voltage
2 | BN/BK | 2105 | Front End Sensor - Left - Voltage | 2 | BN/BK | 2105 | Front End Sensor - Left - Voltage
3 | RD-YE | 753 | Side Impact Sensor - Driver Voltage (w/Side Air Bags) | 3 | PK | 753 | Side Impact Sensor - Driver Voltage (w/Side Air Bags)
4 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage (w/Side Air Bags | 4 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage (w/Side Air Bags
5 | PK | 1184 | Seat Belt Pretensioner - Driver - Low Control | 5 | YE/D-BU | 1184 | Seat Belt Pretensioner - Driver - Low Control
6 | D-GN/WH | 2104 | Front End Sensor - Right - Signal | 6 | D-GN/WH | 2104 | Front End Sensor - Right - Signal
7 | L-GN/RD | 2106 | Front End Sensor - Left - Signal | 7 | L-GN/RD | 2106 | Front End Sensor - Left - Signal
8 | BK | 754 | Side Impact Sensor Driver Signal (w/Side Air Bags) | 8 | BK/WH | 754 | Side Impact Sensor Driver Signal (w/Side Air Bags)
9 | BN/WH | 715 | Side Impact Sensor Passenger Signal (w/Side Air Bags) | 9 | BN/WH | 715 | Side Impact Sensor Passenger Signal (w/Side Air Bags)
10 | D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger - Low Control | 10 | RD/BK | 1187 | Seat Belt Pretensioner - Passenger - Low Control
11 | PK/BK | 1186 | Seat Belt Pretensioner - Passenger - High Control | 11 | D-BU/WH | 1186 | Seat Belt Pretensioner - Passenger - High Control
12 | D-BU | 1185 | Seat Belt Pretensioner - Driver - High Control | 12 | PU | 1185 | Seat Belt Pretensioner - Driver - High Control

#### C302 - I/P Harness to Console Harness

Connector Part Information |

• | AMP 175658

• | 6-Way F 070 MLC W-W PLUG HSG 6P (WH)

Connector Part Information

• | AMP 175657

• | 6-Way M .070 SRS MLC 6POS (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 243 | Ignition 3 Voltage | 1 | YE | 243 | Ignition 3 Voltage
2 | BK | 1050 | Ground | 2 | BK | 1050 | Ground
3 | D-GN/WH | 1135 | Transmission Hold Signal | 3 | D-GN/WH | 1135 | Transmission Hold Signal
4 | BK | 1050 | Ground | 4 | BK | 1050 | Ground
5 | BN/WH | 309 | Right Park Lamp Supply Voltage | 5 | BN/WH | 309 | Right Park Lamp Supply Voltage
BN/WH | 309 | Right Park Lamp Supply Voltage
6 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal | 6 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal

#### C351 - Floor Harness to Left Front Door Harness (LHD)

Connector Part Information |

• | AMP 936283-1

• | 33-Way F 090/JPT 33P Plug Assembly (WH)

Connector Part Information

• | AMP 936280

• | 33-Way M .090/JPT 33P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 201 | Left Front Speaker Output (+) | 1 | PU | 201 | Left Front Speaker Output (+)
2 | GY/WH | 118 | Left Front Speaker Output (-) | 2 | GY/WH | 118 | Left Front Speaker Output (-)
3 | YE | 356 | Driver Door Lock Relay Unlock Control | 3 | WH | 356 | Driver Door Lock Relay Unlock Control
4 | WH | 194 | Door Unlock Control | 4 | WH | 194 | Door Unlock Control
5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal | 5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal | 6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
7 | GY/BK | 90 | Passenger Mirror Motor Left Control | 7 | GY | 90 | Passenger Mirror Motor Left Control
8 | PU/WH | 889 | Passenger Mirror Motor Down Control | 8 | PU/WH | 889 | Passenger Mirror Motor Down Control
9 | RD/WH | 881 | Passenger Mirror Motor Right Control | 9 | RD/WH | 881 | Passenger Mirror Motor Right Control
10 | RD | 581 | Power Window Supply Voltage - Driver Door | 10 | RD | 581 | Power Window Supply Voltage - Driver Door
11 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control | 11 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
12 | D-BU | 1307 | Power Window Master Switch Lockout Control | 12 | D-BU | 1307 | Power Window Master Switch Lockout Control
13 | L-BU | 195 | Door Lock Control | 13 | L-BU/BK | 195 | Door Lock Control
14 | PU/RD | 169 | Power Window Master Switch Left Rear Down Signal | 14 | PU/RD | 169 | Power Window Master Switch Left Rear Down Signal
15 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | 15 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
16 | BN | 253 | Trunk Release Relay Control | 16 | BN | 253 | Trunk Release Relay Control
17 | OG | 640 | Battery Positive Voltage | 17 | OG | 640 | Battery Positive Voltage
18 | BN/BK | 641 | Ignition 3 Voltage | 18 | BN | 141 | Ignition 3 Voltage
BN
19 | BK | 1150 | Ground | 19 | BK | 1150 | Ground
20 | BK | 1150 | Ground | 20 | BK | 1150 | Ground
21 | OG | 580 | Power Window Supply Voltage | 21 | OG | 580 | Power Window Supply Voltage
22 | GY | 1118 | Left Speaker Output (+) Optional | 22 | D-GN | 1118 | Left Speaker Output (+) Optional
23 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal | 23 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal
24 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | 24 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors) | 25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors)
26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors) | 26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors)
27 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | 27 | OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
28 | GY | 295 | Door Lock Actuator Lock Control | 28 | GY | 295 | Door Lock Actuator Lock Control
29 | L-GN | 1370 | Driver Door Lock Switch Signal | 29 | L-GN | 1370 | Driver Door Lock Switch Signal
30 | PU/WH | 294 | Door Lock Actuator Unlock Control | 30 | PU/WH | 294 | Door Lock Actuator Unlock Control
31 | BN/WH | 1201 | Left Speaker Output (-) Optional | 31 | PU | 1201 | Left Speaker Output (-) Optional
32 | YE/GN | 749 | Security Indicator Control (w/Alarm) | 32 | YE | 749 | Security Indicator Control (w/Alarm)
33 | GY/RD | 2232 | Folding Mirror Switch Signal (w/Folding Mirrors) | 33 | GY/BK | 2232 | Folding Mirror Switch Signal (w/Folding Mirrors)

#### C351 - Floor Harness to Left Front Door Harness (RHD)

Connector Part Information |

• | AMP 936283-1

• | 33-Way F 090/JPT 33P Plug Assembly (WH)

Connector Part Information

• | AMP 936280

• | 33-Way M .090/JPT 33P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 201 | Left Front Speaker Output (+) | 1 | L-GN | 201 | Left Front Speaker Output (+)
2 | GY/WH | 118 | Left Front Speaker Output (-) | 2 | D-GN | 118 | Left Front Speaker Output (-)
3-4 | -- | -- | Not Used | 3 | -- | -- | Not Used
5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal | 5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal | 6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
7 | GY/BK | 90 | Passenger Mirror Motor Left Control | 7 | GY/BK | 90 | Passenger Mirror Motor Left Control
8 | PU/WH | 889 | Passenger Mirror Motor Down Control | 8 | PU/WH | 889 | Passenger Mirror Motor Down Control
9 | RD/WH | 881 | Passenger Mirror Motor Right Control | 9 | RD/WH | 881 | Passenger Mirror Motor Right Control
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | BK | 350 | Ground (Hatchback) | 11 | BK | 350 | Ground (Hatchback)
BK | 1150 | Ground (Notchback) | BK | 1150 | Ground (Notchback)
12 | D-BU | 1307 | Power Window Master Switch Lockout Control | 12 | D-BU | 1307 | Power Window Master Switch Lockout Control
13-24 | -- | -- | Not Used | 13-24 | -- | -- | Not Used
25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors) | 25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors)
26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors) | 26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors)
27 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | 27 | OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
28 | GY | 295 | Door Lock Actuator Lock Control | 28 | GY | 295 | Door Lock Actuator Lock Control
29 | PU | 1371 | Passenger Door Lock Switch Signal | 29 | PU | 1371 | Passenger Door Lock Switch Signal
30 | PU/WH | 294 | Door Lock Actuator Unlock Control | 30 | PU/WH | 294 | Door Lock Actuator Unlock Control
31-33 | -- | -- | Not Used | 31-33 | -- | -- | Not Used

#### C361 - Floor Harness to Right Front Door Harness (LHD)

Connector Part Information |

• | AMP 936283-1

• | 33-Way F 090/JPT 33P Plug Assembly (WH)

Connector Part Information

• | AMP 936280

• | 33-Way M .090/JPT 33P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-GN | 200 | Right Front Speaker Output (+) | 1 | L-GN | 200 | Right Front Speaker Output (+)
2 | D-GN | 117 | Right Front Speaker Output (-) | 2 | D-GN | 117 | Right Front Speaker Output (-)
3-4 | -- | -- | Not Used | 3-4 | -- | -- | Not Used
5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal | 5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal | 6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
7 | GY/BK | 90 | Passenger Mirror Motor Left Control | 7 | GY/BK | 90 | Passenger Mirror Motor Left Control
8 | PU/WH | 889 | Passenger Mirror Motor Down Control | 8 | PU/WH | 889 | Passenger Mirror Motor Down Control
9 | RD/WH | 881 | Passenger Mirror Motor Right Control | 9 | RD/WH | 881 | Passenger Mirror Motor Right Control
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | BK | 350 | Ground | 11 | BK | 350 | Ground
12 | D-BU | 1307 | Power Window Master Switch Lockout Control | 12 | D-BU | 1307 | Power Window Master Switch Lockout Control
13-24 | -- | -- | Not Used | 10 | -- | -- | Not Used
25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors) | 25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors)
26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors) | 26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors)
27 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | 27 | OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
28 | GY | 295 | Door Lock Actuator Lock Control | 28 | GY | 295 | Door Lock Actuator Lock Control
29 | PU | 1371 | Driver Door Lock Switch Signal | 29 | PU | 1371 | Driver Door Lock Switch Signal
30 | PU/WH | 294 | Door Lock Actuator Unlock Control | 30 | PU/WH | 294 | Door Lock Actuator Unlock Control
31-33 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C361 - Floor Harness to Right Front Door Harness (RHD)

Connector Part Information |

• | AMP 936283-1

• | 33-Way F 090/JPT 33P Plug Assembly (WH)

Connector Part Information

• | AMP 936280

• | 33-Way M .090/JPT 33P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 200 | Right Front Speaker Output (+) | 1 | PU | 200 | Right Front Speaker Output (+)
2 | GY/WH | 117 | Right Front Speaker Output (-) | 2 | GY/WH | 117 | Right Front Speaker Output (-)
3 | YE | 356 | Driver Door Lock Relay Unlock Control | 3 | WH | 356 | Driver Door Lock Relay Unlock Control
4 | WH | 194 | Door Unlock Control | 4 | WH | 194 | Door Unlock Control
5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal | 5 | PU | 167 | Power Window Master Switch Passenger Front Down Signal
6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal | 6 | L-BU | 166 | Power Window Master Switch Passenger Front Up Signal
7 | GY/BK | 90 | Passenger Mirror Motor Left Control | 7 | GY/BK | 90 | Passenger Mirror Motor Left Control
8 | PU/WH | 889 | Passenger Mirror Motor Down Control | 8 | PU/WH | 889 | Passenger Mirror Motor Down Control
9 | RD/WH | 881 | Passenger Mirror Motor Right Control | 9 | RD/WH | 881 | Passenger Mirror Motor Right Control
10 | RD | 581 | Power Window Supply Voltage - Driver Door | 10 | RD | 581 | Power Window Supply Voltage - Driver Door
11 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control | 11 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
BK | 350 | Ground | BK | 350 | Ground
12 | D-BU | 1307 | Power Window Master Switch Lockout Control | 12 | D-BU | 1307 | Power Window Master Switch Lockout Control
13 | L-BU | 195 | Door Lock Control | 13 | L-BU | 195 | Door Lock Control
14 | PU/RD | 169 | Power Window Master Switch Left Rear Down Signal | 14 | PU/RD | 169 | Power Window Master Switch Left Rear Down Signal
15 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | 15 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
16 | BN | 253 | Trunk Release Relay Control | 16 | BN | 253 | Trunk Release Relay Control
17 | OG | 640 | Battery Positive Voltage | 17 | OG | 640 | Battery Positive Voltage
18 | BN/BK | 641 | Ignition 3 Voltage | 18 | BN | 641 | Ignition 3 Voltage
19 | BK | 350 | Ground | 19 | BK | 1150 | Ground
20 | BK | 350 | Ground | 20 | BK | 1150 | Ground
21 | OG | 580 | Power Window Supply Voltage | 21 | OG | 580 | Power Window Supply Voltage
22 | D-GN | 1118 | Left Speaker Output (+) Optional | 22 | D-GN | 1118 | Left Speaker Output (+) Optional
23 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal | 23 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal
24 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | 24 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors) | 25 | L-GN/BK | 2231 | Folding Mirror Motor Extend Control (w/Folding Mirrors)
26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors) | 26 | BN/WH | 2230 | Folding Mirror Motor Retract Control (w/Folding Mirrors)
27 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | 27 | OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
28 | GY | 295 | Door Lock Actuator Lock Control | 28 | GY | 295 | Door Lock Actuator Lock Control
29 | L-GN | 1370 | Driver Door Lock Switch Signal | 29 | L-GN | 1370 | Driver Door Lock Switch Signal
30 | PU/WH | 294 | Door Lock Actuator Unlock Control | 30 | PU/WH | 294 | Door Lock Actuator Unlock Control
31 | PU | 1201 | Left Speaker Output (-) Optional | 31 | PU | 1201 | Left Speaker Output (-) Optional
32 | YE/D-GN | 749 | Security Indicator Control (w/Alarm) | 32 | YE | 749 | Security Indicator Control (w/Alarm)
33 | GY/RD | 2232 | Folding Mirror Switch Signal (w/Folding Mirrors) | 33 | GY/BK | 2232 | Folding Mirror Switch Signal (w/Folding Mirrors)

#### C371 - Floor Harness to Left Rear Door Harness

Connector Part Information |

• | AMP 85218-1

• | 11-Way F 070/110 Series 11P Plug Housing (WH)

Connector Part Information

• | AMP 85216

• | 11-Way M 070/110 Series 11P Cap Housing (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 116 | Left Rear Speaker Output (-) | 1 | D-GN | 116 | Left Rear Speaker Output (-)
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | BN | 199 | Left Rear Speaker Output (+) | 4 | BN | 199 | Left Rear Speaker Output (+)
L-GN | 199 | Left Rear Speaker Output (+) (Except North America)
5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (w/Power Windows) | 5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (w/Power Windows)
6 | D-BU | 1307 | Power Window Master Switch Lockout Control (w/Power Windows) | 6 | D-BU | 1307 | Power Window Master Switch Lockout Control (w/Power Windows)
7 | PU/RD | 169 | Power Window Master Switch Left Rear Down Signal (w/Power Windows) | 7 | PU | 169 | Power Window Master Switch Left Rear Down Signal (w/Power Windows)
8 | GY | 295 | Door Lock Actuator Lock Control | 8 | GY | 295 | Door Lock Actuator Lock Control
9 | BK | 1250 | Ground (w/Power Windows) | 9 | BK | 1250 | Ground (w/Power Windows)
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | PU/WH | 294 | Door Lock Actuator Unlock Control | 11 | PU | 294 | Door Lock Actuator Unlock Control
PU | 294 | Door Lock Actuator Unlock Control (Except North America)

#### C381 - Floor Harness to Right Rear Door Harness

Connector Part Information |

• | AMP 85218-1

• | 11-Way F 070/110 Series 11P Plug Housing (WH)

Connector Part Information

• | AMP 85216

• | 11-Way M 070/110 Series 11P Cap Housing (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-BU | 115 | Right Rear Speaker Output (-) | 1 | D-GN | 115 | Right Rear Speaker Output (-)
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | D-BU/WH | 46 | Right Rear Speaker Output (+) | 4 | BN | 199 | Right Rear Speaker Output (+)
5 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (w/Power Windows) | 5 | D-GN | 168 | Power Window Master Switch Right Rear Up Signal (w/Power Windows)
6 | D-BU | 1307 | Power Window Master Switch Lockout Control (w/Power Windows) | 6 | D-BU | 1307 | Power Window Master Switch Lockout Control (w/Power Windows)
7 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal (w/Power Windows) | 7 | PU | 169 | Power Window Master Switch Right Rear Down Signal (w/Power Windows)
8 | GY | 295 | Door Lock Actuator Lock Control | 8 | GY | 295 | Door Lock Actuator Lock Control
9 | BK | 350 | Ground (w/Power Windows) | 9 | BK | 1250 | Ground (w/Power Windows)
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | PU/WH | 294 | Door Lock Actuator Unlock Control | 11 | PU | 294 | Door Lock Actuator Unlock Control

#### C391 - Rear ABS Harness to Left Rear Wheel Speed Sensor Jumper

Connector Part Information |

• | Bosch 2264-420424 (F)

• | 2-Way F Connector (BK)

Connector Part Information

• | Bosch 2264-420424 (M)

• | 2-Way M Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 885 | Left Rear Wheel Speed Sensor Signal | 1 | WH | 885 | Left Rear Wheel Speed Sensor Signal
2 | GY | 884 | Left Rear Wheel Speed Sensor Low Reference | 2 | BK | 884 | Left Rear Wheel Speed Sensor Return

#### C392 - Rear ABS Harness to Right Rear Wheel Speed Sensor Jumper

Connector Part Information |

• | Bosch 2264-420424 (F)

• | 2-Way F Connector (BK)

Connector Part Information

• | Bosch 2264-420424 (M)

• | 2-Way M Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 883 | Right Rear Wheel Speed Sensor Signal | 1 | WH | 883 | Right Rear Wheel Speed Sensor Signal
2 | GY | 882 | Right Rear Wheel Speed Sensor Low Reference | 2 | BK | 882 | Right Rear Wheel Speed Sensor Return

#### C401 - Trunk Harness to Floor Harness (Hatchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America) | 1 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | YE | 20 | Stop Lamp Supply Voltage | 3 | L-BU | 20 | Stop Lamp Supply Voltage
4 | PK/BK | 1846 | Ignition 1 Voltage (North America) | 4 | PK/BK | 1846 | Ignition 1 Voltage
5 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 5 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
6 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 6 | L-BU/BK | 14 | Left Turn Signal Lamp Supply Voltage
7 | PU | 709 | Left Park Lamp Supply Voltage | 7 | PU/BK | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage
8 | BN/WH | 309 | Right Park Lamp Supply Voltage | 8 | BN/WH | 309 | Right Park Lamp Supply Voltage
BN/WH | 309 | Right Park Lamp Supply Voltage

#### C401 - Trunk Harness to Floor Harness (Notchback)

Connector Part Information |

• | AMP 936233

• | 8-Way F 090III 8P Plug Assembly (WH)

Connector Part Information

• | AMP 936242-1

• | 8-Way M 090III 8P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 1 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
2 | BN/WH | 309 | Right Park Lamp Supply Voltage | 2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | YE | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 3 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU/WH | 709 | Left Park Lamp Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
L-BU/BK
6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America) | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America)
7 | L-GN | 24 | Backup Lamp Supply Voltage | 7 | L-GN | 24 | Backup Lamp Supply Voltage
8 | PK/BK | 1846 | Ignition 1 Voltage (North America) | 8 | PK/BK | 1846 | Ignition 1 Voltage (North America)
YE/BK | 2001 | GPS (Optional) | YE/BK | 2001 | GPS (Optional)

#### C401 - Trunk Harness to Floor Harness (Optional)

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641053

• | 6-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 2 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
3 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 3 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
4 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 4 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
5 | PU/BK | 709 | Left Park Lamp Supply Voltage | 5 | PU/BK | 709 | Left Park Lamp Supply Voltage
6 | BN/WH | 309 | Right Park Lamp Supply Voltage | 6 | BN/WH | 309 | Right Park Lamp Supply Voltage

#### C401 - Trunk Harness to Floor Harness (Notchback) (Optional)

Connector Part Information |

• | AMP 936092

• | 10-Way F 090III 8P Plug Assembly (WH)

Connector Part Information

• | AMP 636129

• | 10-Way M 090III 8P CAP Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 1 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
2 | BN/WH | 309 | Right Park Lamp Supply Voltage | 2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | YE | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 3 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU/WH | 709 | Left Park Lamp Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 5 | L-BU/BK | 14 | Left Turn Signal Lamp Supply Voltage
6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
7 | L-GN | 24 | Backup Lamp Supply Voltage | 7 | L-GN | 24 | Backup Lamp Supply Voltage
8 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America) | 8 | L-BU/PU | 1986 | EVAP Canister Vent Solenoid Control (North America)
9 | PK/BK | 1846 | Ignition 1 Voltage (North America) | 9 | PK/BK | 1846 | Ignition 1 Voltage (North America)
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C402 - Trunk Lid Harness to Floor Harness (Notchback)

Connector Part Information |

• | AMP 174923

• | 6-Way F 070 Multi Lock Connector (WH)

Connector Part Information

• | AMP 174930

• | 6-Way M .070 SRS MLC 6POS (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal (w/RKE) | 1 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal (w/RKE)
2 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 2 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
3 | BK | 1250 | Ground | 3 | BK | 1250 | Ground
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU/BK | 709 | Left Park Lamp Supply Voltage
PU/WH
5 | BN | 253 | Trunk Release Relay Control | 5 | BN | 253 | Trunk Release Relay Control
6 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal (w/RKE) | 6 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal (w/RKE)

#### C403 - Liftgate Jumper Harness to Floor Harness (Notchback)

Connector Part Information |

• | AMP 651038

• | 4-Way F 070 Multi Lock Connector (WH)

Connector Part Information

• | AMP 641041

• | 4-Way M .070 SRS MLC 6POS (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 750 | Ground | 1 | BK | 750 | Ground
2 | BK | 750 | Ground | 2 | BK | 750 | Ground
3 | PU | 293 | Rear Compartment Lid Ajar Switch Signal (w/RKE) | 3 | PU | 293 | Rear Compartment Lid Ajar Switch Signal (w/RKE)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### C403 - Liftgate Jumper Harness to Floor Harness (Hatchback)

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU/WH | 709 | Left Park Lamp Supply Voltage
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | L-GN | 24 | Backup Lamp Supply Voltage
L-GN | 24 | Backup Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 5 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 6 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)

#### C404 - Liftgate Jumper Harness to Floor Harness (Notchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 393 | Rear Window Wiper Motor Control | 1 | WH | 393 | Rear Window Wiper Motor Control
2 | BN | 441 | Ignition 3 Voltage | 2 | RD/D-BU | 441 | Ignition 3 Voltage
3 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 3 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
4 | PK/BK | 1303 | Liftgate Switch Signal (w/RKE) | 4 | PK/BK | 1303 | Liftgate Switch Signal (w/RKE)
5 | L-BU | 263 | Rear Compartment Lid Ajar Switch (w/RKE) | 5 | L-BU | 263 | Rear Compartment Lid Ajar Switch (w/RKE)
6 | PU | 294 | Door Lock Actuator Unlock Control | 6 | PU | 294 | Door Lock Actuator Unlock Control
7 | GY | 295 | Door Lock Actuator Lock Control | 7 | GY | 295 | Door Lock Actuator Lock Control
8 | PU | 709 | Left Park Lamp Supply Voltage | 8 | PU | 709 | Left Park Lamp Supply Voltage

#### C404 - Liftgate Jumper Harness to Floor Harness (Hatchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 294 | Door Lock Actuator Unlock Control | 1 | PU/WH | 294 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control | 2 | GY | 295 | Door Lock Actuator Lock Control
3 | L-BU | 263 | Rear Compartment Lid Ajar Switch (w/RKE) | 3 | L-BU | 263 | Rear Compartment Lid Ajar Switch (w/RKE)
4 | PK/BK | 1303 | Liftgate Switch Signal (w/RKE) | 4 | PK/BK | 1303 | Liftgate Switch Signal (w/RKE)
5 | BN | 441 | Ignition 3 Voltage | 5 | RD/D-BU | 441 | Ignition 3 Voltage
6 | WH | 393 | Rear Window Wiper Motor Control | 6 | WH | 393 | Rear Window Wiper Motor Control
7 | PU | 293 | Rear Defog Element Supply Voltage | 7 | PU | 293 | Rear Defog Element Supply Voltage
D-GN
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C405 - Liftgate Jumper Harness to Liftgate Harness (Hatchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 750 | Ground | 2 | BK | 750 | Ground
3 | BK | 750 | Ground | 3 | BK | 750 | Ground
4 | L-GN | 24 | Backup Lamp Supply Voltage | 4 | L-GN | 24 | Backup Lamp Supply Voltage
L-GN | 24 | Backup Lamp Supply Voltage
5 | L-BU | 20 | Stop Lamp Supply Voltage | 5 | L-BU | 20 | Stop Lamp Supply Voltage
6 | BN | 441 | Ignition 3 Voltage | 6 | PK | 441 | Ignition 3 Voltage
7 | WH | 393 | Rear Window Wiper Motor Control | 7 | WH | 393 | Rear Window Wiper Motor Control
8 | BK | 750 | Ground | 8 | BK | 750 | Ground

#### C405 - Liftgate Jumper Harness to Liftgate Harness (Notchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 393 | Rear Window Wiper Motor Control | 1 | WH | 393 | Rear Window Wiper Motor Control
2 | BN | 441 | Ignition 3 Voltage | 2 | RD/BU | 441 | Ignition 3 Voltage
3 | L-BU | 20 | Stop Lamp Supply Voltage | 3 | L-BU | 20 | Stop Lamp Supply Voltage
4 | PK/BK | 1303 | Liftgate Switch Signal | 4 | PK/BK | 1303 | Liftgate Switch Signal
5 | L-BU | 263 | Rear Compartment Lid Ajar Switch | 5 | L-BU | 263 | Rear Compartment Lid Ajar Switch
6 | PU | 294 | Door Lock Actuator Unlock Control | 6 | PU | 294 | Door Lock Actuator Unlock Control
7 | GY | 295 | Door Lock Actuator Lock Control | 7 | GY | 295 | Door Lock Actuator Lock Control
8 | PU | 709 | Left Park Lamp Supply Voltage | 8 | PU | 709 | Left Park Lamp Supply Voltage

#### C406 - Liftgate Jumper Harness to Liftgate Harness (Hatchback)

Connector Part Information |

• | AMP 936230-1

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 1 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
2 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal (w/RKE) | 2 | PK/BK | 1303 | Rear Compartment Lid Ajar Switch Signal (w/RKE)
3 | D-GN | 293 | Rear Defog Element Supply Voltage | 3 | D-GN | 293 | Rear Defog Element Supply Voltage
PU (North America)
4 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal (w/RKE) | 4 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal (w/RKE)
5 | PU | 294 | Door Unlock Actuator Control | 1 | PU | 294 | Door Unlock Actuator Control
6 | GY | 295 | Door Lock Actuator Control | 2 | GY | 295 | Door Lock Actuator Control

#### C406 - Liftgate Jumper Harness to Liftgate Harness (Notchback)

Connector Part Information |

• | KET MG 651038

• | 4-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641041

• | 4-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 750 | Ground | 1 | BK | 750 | Ground
2 | BK | 750 | Ground | 2 | BK | 750 | Ground
3 | PU | 293 | Rear Defog Element Supply Voltage | 3 | PU | 293 | Rear Defog Element Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### C407 - Trunk Harness to Left Tail Lamp Jumper Harness (Hatchback)

Connector Part Information |

• | KET MG 610047

• | 4-Way F 250 Series (WH)

Connector Part Information

• | KET MG 620046

• | 4-Way M 250 Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
WH/D-BU (North America)
2 | YE | 20 | Stop Lamp Switch Signal | 2 | YE | 20 | Stop Lamp Switch Signal
RD (North America)
3 | BK | 550 | Ground | 3 | BK | 550 | Ground
BK | 550 | Ground
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage

#### C408 - Trunk Harness to Right Tail Lamp Jumper Harness (Hatchback)

Connector Part Information |

• | KET MG 610047

• | 4-Way F 250 Series (WH)

Connector Part Information

• | KET MG 620046

• | 4-Way M 250 Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | WH/D-GN | 309 | Right Park Lamp Supply Voltage
2 | YE | 20 | Stop Lamp Switch Signal | 2 | RD | 20 | Stop Lamp Switch Signal
3 | BK | 550 | Ground | 3 | BK | 550 | Ground
BK/WH (North America) | 550 | Ground
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Right Turn Signal Lamps Supply Voltage

#### C417 - Trunk Harness to Left Side Marker Lamp Jumper Harness

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | WH | 709 | Left Park Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground

#### C418 - Trunk Harness to Right Side Marker Lamp Jumper Harness

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground

#### C420 - Tailgate Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Hatchback)

Connector Part Information |

• | KET MG 610398

• | 6-Way F SDL Series (WH)

Connector Part Information

• | KET MG 620401

• | 6-Way M Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 750 | Ground | 1 | BK/WH | 550 | Ground
2 | BK | 750 | Ground | 2 | BK | 550 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | RD | 122 | Rear Fog Lamp Supply Voltage (Except North America) | 4 | RD | 122 | Rear Fog Lamp Supply Voltage (Except North America)
5 | L-BU | 20 | Stop Lamp Switch Signal | 5 | RD | 20 | Stop Lamp Switch Signal
6 | PU | 709 | Park Lamp | 6 | WH/D-GN | 709 | Park Lamp

#### C420 - Tailgate Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Notchback)

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series

Connector Part Information

• | KET MG 642449

• | 6-Way M 090 II Series

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RD | 122 | Rear Fog Lamp Supply Voltage | 1 | WH | 122 | Rear Fog Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
BK | 550 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | D-BU | 15 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Left Turn Signal Lamps Supply Voltage
5 | BN/WH | 309 | Left Park Lamp Supply Voltage | 5 | WH/BK | 309 | Left Park Lamp Supply Voltage
6 | YE | 20 | Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Switch Signal

#### C421 - Tailgate Harness to Left Backup Lamp/Tail Lamp Jumper Harness (Notchback)

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series

Connector Part Information

• | KET MG 642449

• | 6-Way M 090 II Series

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RD | 122 | Rear Fog Lamp Supply Voltage | 1 | RD | 122 | Rear Fog Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | WH/D-GN | 709 | Left Park Lamp Supply Voltage
6 | YE | 20 | Stop Lamp Switch Signal | 6 | YE | 20 | Stop Lamp Switch Signal

#### C421 - Tailgate Harness to Left Backup Lamp and Tail Lamp Jumper Harness (Hatchback)

Connector Part Information |

• | KET MG 610398

• | 6-Way F SDL Series (WH)

Connector Part Information

• | KET MG 620401

• | 6-Way M Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 750 | Ground | 1 | BK/WH | 550 | Ground
2 | BK | 750 | Ground | 2 | BK | 550 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 4 | RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
5 | L-BU | 20 | Stop Lamp Switch Signal | 5 | RD | 20 | Stop Lamp Switch Signal
6 | PU | 709 | Park Lamp | 6 | WH/D-GN | 709 | Park Lamp

#### C422 Tailgate Harness to License Lamps Jumper Harness (Hatchback)

Connector Part Information |

• | KET MG 610489

• | 2-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620490

• | 2-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 750 | Ground | 1 | WH | 750 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage | 2 | BK | 709 | Left Park Lamp Supply Voltage

#### C422 Tailgate Harness to License Lamps Jumper Harness (Notchback)

Connector Part Information |

• | KET MG 610489

• | 2-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620490

• | 2-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | BK | 709 | Left Park Lamp Supply Voltage
2 | BK | 1250 | Ground | 2 | WH | 1250 | Ground

#### C423 - Floor Harness to Left Backup Lamp/Tail Lamp Jumper Harness (Optional)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 650 | Ground | 1 | BK | 650 | Ground
2 | BK | 650 | Ground | 2 | BK | 650 | Ground
3 | BK | 650 | Ground | 3 | BK | 650 | Ground
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU | 709 | Left Park Lamp Supply Voltage
5 | L-BU | 20 | Stop Lamp Switch Signal | 5 | L-BU | 20 | Stop Lamp Switch Signal
6 | L-GN | 24 | Backup Lamp Supply Voltage | 6 | L-GN | 24 | Backup Lamp Supply Voltage
7 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 7 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
8 | RD | 122 | Rear Fog Lamp Supply Voltage | 8 | RD | 122 | Rear Fog Lamp Supply Voltage

#### C424 - Floor Harness to Right Backup Lamp/Tail Lamp Jumper Harness (Optional)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 550 | Ground | 1 | BK | 550 | Ground
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | BK | 550 | Ground | 3 | BK | 550 | Ground
4 | BN/WH | 309 | Left Park Lamp Supply Voltage | 4 | BN/WH | 309 | Left Park Lamp Supply Voltage
5 | L-BU | 20 | Stop Lamp Switch Signal | 5 | L-BU | 20 | Stop Lamp Switch Signal
6 | L-GN | 24 | Backup Lamp Supply Voltage | 6 | L-GN | 24 | Backup Lamp Supply Voltage
7 | D-BU | 15 | Left Turn Signal Lamp Supply Voltage | 7 | D-BU | 15 | Left Turn Signal Lamp Supply Voltage
8 | RD | 122 | Rear Fog Lamp Supply Voltage | 8 | RD | 122 | Rear Fog Lamp Supply Voltage

#### C425 - Floor Harness to Left Side Marker Lamp Jumper Harness (Optional)

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | WH | 709 | Left Park Lamp Supply Voltage
2 | BK | 650 | Ground | 2 | BK | 650 | Ground

#### C426 - Floor Harness to Right Side Marker Lamp Jumper Harness (Optional)

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground