For 1990-2009 cars

Component | Pass Through Pins | Resistance in Ohms 20°C (68°F) | Resistance in Ohms 140°C (284°F)
--- | --- | --- | ---
Solenoid 1 | 3, 12 | 26-27 | 26-345, not relative to temperature
Solenoid 2 | 3, 13 | 26-27 | 26-345, not relative to temperature
Pressure Control Solenoid Valve - (PCS) 3 | 5, 6 | 5.25-6.15 | 5.3-6.3, not relative to temperature
Pressure Control Solenoid Valve - (PCS) 4 | 5, 7 | 5.25-6.15 | 5.3-6.3, not relative to temperature
Pressure Control Solenoid Valve - (PCS) 5 | 5, 10 | 5.25-6.15 | 5.3-6.3, not relative to temperature
Pressure Control Solenoid Valve - (PCS) 6 | 5, 11 | 5.25-6.15 | 5.3-6.3, not relative to temperature
Transaxle Temperature Sensor¹ | 4, 9 | -- | 980-1,000
Input Speed Sensor | 15, 16 | 825-835 | 788-871, not relative to temperature
Output Speed Sensor¹ | 1, 2 | ∞ | ∞
¹ The resistance of the transaxle is necessarily dependent on the temperature