For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the floor console. Refer to Front Floor Console Replacement.
3. Disconnect the wiring harness connectors from the shift control lever.
4. Loosen the control cable adjusting nut.
5. Disconnect the control cable from the shift control lever assembly.
6. Remove the shift control lever assembly mounting bolts and nuts.
7. Remove the shift control lever assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the shift control lever assembly with themounting bolts and nuts and tighten to 8 N·m (71 lb in).
2. Connect the control cable to the shift control lever assembly.
3. Install the control cable adjusting nut and tighten to 8 N·m (71 lb in).
4. Connect the harness connector.
5. Adjust the control cable. Refer to Shift Control Cable Adjustment.
6. Install the floor console. Refer to Front Floor Console Replacement.
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.