For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the trailing link-to-trailing link bracket nut and the bolt.
3. Remove the trailing link bracket-to-body bolts.
4. Remove the trailing link bracket.

### Installation Procedure

1. Install the trailing link bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the trailing link bracket-to-body bolts and tighten to 70 N·m (52 lb ft).
3. Connect the trailing link to the trailing link bracket by installing the bolt and the trailing link-to-trailing link bracket nut and tighten to 100 N·m (74 lb ft).
4. Lower the vehicle.