For 1990-2009 cars

1. Apply automatic transmission fluid to the new forward clutch accumulator piston fluid seal ring (613).
2. Install the new forward clutch accumulator piston fluid seal ring (613) onto forward clutch accumulator piston (612).
3. Install the forward clutch accumulator piston spring (614) and the forward clutch accumulator piston (612) into the forward clutch accumulator cover (616).
4. Apply automatic transmission fluid to the new forward clutch accumulator cover seal (615).
5. Install the new forward clutch accumulator cover seal (615) onto forward clutch accumulator cover (616).
6. Install the forward clutch accumulator cover assembly onto the transmission case cover.

Caution: Refer to Fastener Caution in the Preface section.

7. Install one of the two forward clutch accumulator cover bolts (617) and tighten to 10 N·m (89 lb in).
8. Apply automatic transmission fluid to the 3 new forward clutch housing fluid seal rings (607).

Install the 3 new forward clutch housing fluid seal rings (607).

9. Install the forward/direct clutch housing thrust selective bearing race (628) without any markings. This is the 0.81 mm (0.032 in) thick race and will determine the correct thickness for the forward/direct clutch end play measurement.
10. Apply automatic transmission fluid to the 2 new 4-5 clutch apply pipe seals (608).
11. Install the 2 pipe seals (608) onto the 4-5 clutch apply pipe (609).

Note: Do not damage the pipe seals or the 4-5 clutch apply pipe.

12. Using a plastic hammer if needed, install the 4-5 clutch apply pipe (609) into the transmission case cover.
13. Install the two, 4-5 clutch apply pipe retainers (610).
14. Install the four, 4-5 clutch apply pipe bolts (611) and tighten to 7 N·m (62 lb in).