For 1990-2009 cars

#### Tools Required

DT 46473 (DW260-050) Park/Neutral Position Switch Installer

### Removal Procedure

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector from the park/neutral position switch.
3. Disconnect the shift control cable and the retaining clip.
4. Remove the shift lever nut and the shift lever.
5. Remove the park/neutral start switch.

### Installation Procedure

1. Place the shift lever in Neutral.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the park/neutral start switch.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Use DT 46473 (1) to adjust the start switch.
4. Install the shift lever and the shift lever nut.

Tighten
Tighten the nut to 10 N·m (89 lb in).

5. Connect the shift control cable and the retaining clip.
6. Connect the electrical connector to the park/neutral position switch.
7. Connect the negative battery cable.