For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Remove the front bumper energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement .
4. Remove the bolts and the front bumper impact bar.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front impact bar with the bolts.

Tighten
Tighten the front impact bar bolts to 39 N·m (29 lb ft).

2. Install the front bumper energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement .
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
4. Connect the electrical connector.