For 1990-2009 cars

### Circuit Description

The speed sensitive power steering (SSPS) control module determines current flow of the power steering fluid flow control valve actuator (solenoid) that is relative to the vehicle speed.

The solenoid converts the electrical signal into a corresponding hydraulic control variable, which determines the amount of reaction pressure and thus the steering force.

### Conditions for Running the DTC

The ignition is ON.

### Conditions for Setting the DTC

Short between the high circuit to the power steering fluid flow control valve actuator

### Action Taken When the DTC Sets

• | The SSPS warning light will illuminate.

• | Power steering assist will default to full power steering effort.

• | The SSPS control module will store a DTC 02 in memory.

### Conditions for Clearing the DTC

• | Conditions for the fault are no longer present.

• | Use the scan tool in order to clear the DTC and cycle the ignition in order to clear the warning lamp.

### Diagnostic Aids

Check for the following conditions if a history or intermittent DTC is indicated.

• | A poor connection at the SSPS control module. Inspect the harness connectors for backed out terminals, improper mating, improperly formed or damaged terminals, and poor terminal to wire connections.

• | A damaged wiring harness. Inspect the wiring harness for damages. If the wiring harness appears to be in good condition, observe the display on the DMM while moving the connectors and wiring harnesses related to the circuits. A change in the DMM display during the test will indicate the location of the fault.

• | For additional information, refer to Testing for Intermittent Conditions and Poor Connections .

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This test checks for a short to voltage in the wiring.

2. This test checks for a poor connection at the SSPS control module.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Power Steering Schematics Connector End View Reference: Component Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Remove the speed sensitive power steering (SSPS) control module.
2. Turn ON the ignition, with the engine OFF.
3. Use a DMM to measure the voltage across the high actuator control circuit of the SSPS control module. Refer to Circuit Testing .

Is the measured resistance greater than the specified value?

0 V

Go to Step 4

Go to Step 3

3 | Test for a poor connection at the SSPS control module. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | -- | Go to Step 6 | Go to Step 5
4 | Repair the short to voltage on the low actuator control circuit of the SSPS control module. Refer to Wiring Repairs . Did you complete the repair? | -- | Go to Step 6 | --
5 | Replace the SSPS control module control module. Refer to Power Steering Control Module Replacement . Is the repair complete? | -- | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2