For 1990-2009 cars

Caution: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result.

1. Remove the gasket (322).
2. Remove the front control valve body spacer plate (321).
3. Remove the gasket (320).
4. Remove the ball check valve (355).
5. Remove the fluid strainer (352).
6. Remove the pressure relief valve (351).
7. Remove the pressure relief valve spring (350).
8. Remove the 2 check valves (360).
9. Remove the 2 check valve compression springs (361).
10. Remove the sleeve/bore plug retainer (349).
11. Remove the solenoid modulator valve bore plug (348).
12. Remove the forward clutch (C1) control valve (354).
13. Remove the sleeve/bore plug retainer (349).
14. Remove the solenoid modulator valve bore plug (348).
15. Remove the neutral relay valve spring (357).
16. Remove the neutral relay valve (356).
17. Remove the sleeve/bore plug retainer (349).
18. Remove the solenoid modulator valve bore plug (348).
19. Remove the second coast clutch (B1) control valve (359).
20. Remove the second coast clutch (B1) control valve spring (358).
21. Remove the sleeve/bore plug retainer (349).
22. Remove the solenoid modulator valve bore plug (348).
23. Remove the solenoid modulator valve spring (347).
24. Remove the solenoid modulator valve (346).