For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror. Refer to Outside Rearview Mirror Replacement.
2. Remove the front door glass. Refer to Front Side Door Window Replacement.
3. Remove the glass run.

### Installation Procedure

1. Install the glass run.
2. Install the front door glass. Refer to Front Side Door Window Replacement.
3. Install the outside rearview mirror. Refer to Outside Rearview Mirror Replacement.