For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headlamp. Refer to Headlamp Replacement.
3. Disconnect the electrical connector.
4. Remove the side marker lamp.

### Installation Procedure

1. Connect the electrical connector.
2. Install the side marker lamp.
3. Install the headlamp. Refer to Headlamp Replacement.
4. Connect the negative battery cable.