For 1990-2009 cars

### Removal Procedure

1. Remove the screws and the sun visor from the headliner.
2. Disconnect the vanity mirror electrical connector.
3. Remove the screw and the sun visor support from the headliner.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the sun visor support to the headliner with the screw.

Tighten
Tighten the sun visor support screw to 1.5 N·m (13 lb in).

2. Connect the vanity mirror electrical connector.
3. Install the sun visor to the headliner with the screws.

Tighten
Tighten the sun visor screws to 4 N·m (35 lb in).