For 1990-2009 cars

Connector 1: | Fuse Block - Underhood Label
Connector 2: | Fuse Block Underhood - Top View
Connector 3: | Fuse Block Underhood - Bottom View
Connector 4: | Fuse Block - Underhood X1
Connector 5: | Fuse Block - Underhood X2
Connector 6: | Fuse Block - Underhood X3
Connector 7: | Fuse Block - Underhood X4
Connector 8: | Fuse Block - Underhood X5
Connector 9: | Fuse Block - Underhood X6
Connector 10: | Fuse Block - Underhood X7
Connector 11: | Fuse Block - Underhood Auxiliary Label
Connector 12: | Fuse Block - I/P Label
Connector 13: | Fuse Block - I/P Top View
Connector 14: | Fuse Block - I/P Bottom View
Connector 15: | Fuse Block - I/P

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

No. | Device | Rating | Description
--- | --- | --- | ---
EF1 | BATT PWR Fuse | 30A | Battery Main, F13-F16, F21-F24
EF2 | ABS Fuse | 60A | EBCM, Oil Feeding Connector
EF3 | HVAC BLWR Fuse | 30A | Blower Relay
EF4 | IGN 2 Fuse | 30A | Ignition Switch - 2
EF5 | IGN 1 Fuse | 30A | Ignition Switch - 1
EF6 | COOL FAN LOW Fuse | 20A | Cooling Fan Low Relay
EF7 | DEFOG Fuse | 30A | Defog Relay
EF8 | COOL FAN HI Fuse | 30A | Cooling Fan HI Relay (Gasoline)
40A | Cooling Fan HI Dummy Plug (Diesel)
EF9 | PWR WINDOW Fuse | 20A | Power Window Switch
EF10 | IGN COIL Fuse | 15A | Fuel Connector, ECM, MR-140, LEGR, EI System
EF11 | ECM Fuse | 10A | ECM, Main Relay, Sirius D4
EF12 | HEADLAMPS Fuse | 25A | Headlamp, ILLUM Relay
EF13 | STOP LAMPS Fuse | 15A | Brake Switch
EF14 | DRIVER'S PWR WNOW Fuse | 20A | Power Window Switch
EF15 | HI BEAM Fuse | 15A | Headlamp HI
EF16 | HORN Fuse | 15A | Horn Relay, Siren, Hood Contact Switch
EF17 | A/C Fuse | 10A | A/C Comp Relay
EF18 | FUEL PUMP Fuse | 15A | Fuel Pump
EF19 | IP FUSE BLOCK Fuse | 15A | Cluster, Key Remind S/W, Folding Mirror Unit, MAP Lamp, Room Lamp, Trunk Open Lamp, Trunk Open Switch
EF20 | LOW BEAM LT Fuse | 10A | Headlamp LO
EF21 | ENG SNSR Fuse | 15A | EVAP Canister Purge Solenoid, HO2S, Cooling Fan Relay
EF22 | INJECTOR Fuse | 15A | Injector, EGR, EEGR
EF23 | ILLUM LT Fuse | 10A | License Plate Lamp, Chime Bell, Tail Lamp, Headlamp
EF24 | FRT FOG Fuse | 15A | Fog Lamp Relay
EF25 | MIR HTD Fuse | 10A | Electric OSRV Mirror
EF26 | DR/LCK Fuse | 15A | Central Door Lock Unit
EF27 | LOW BEAM RT Fuse | 10A | Headlamp LO
EF28 | ILLUM RT Fuse | 10A | ILLUM Circuit, Headlamp, Tail Lamp
EF29 | SPARE | 10A | Not Used
EF30 | SPARE | 15A | Not Used
EF31 | SPARE | 25A | Not Used

### Fuse Block Underhood - Top View

### Fuse Block Underhood - Bottom View

### Fuse Block - Underhood X1

#### Connector Part Information

- OEM: MG612102
- Service: N/A
- Description: 21-Way F Hybrid 1809 Series (WH)

#### Fuse Block - Underhood X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/D-GN | 267 | Heated Mirror Coil Supply Voltage
2 | -- | -- | Not Used
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
4 | 0.5 WH/BK | 193 | Rear Defog Relay Control
5 | 0.5 PU/WH | 709 | Left Park Lamp Supply Voltage
0.5 PU | 709 | Left Park Lamp Supply Voltage (Hatchback/Station Wagon)
6 | 0.5 PU/WH | 709 | Left Park Lamp Supply Voltage (Notchback LHD)
0.5 PU | 709 | Left Park Lamp Supply Voltage (Notchback RHD) (Hatchback LHD)
7 | 0.5 BN | 141 | Ignition 2 Voltage (C60/C66)
0.3 BN | 41 | Ignition 2 Voltage (C68)
8 | 0.5 L-GN | 876 | Rough Road Signal w/ ABS
9 | 1.25 OG | 140 | Battery Positive Voltage
10 | 0.5 BN/WH | 309 | Right Park Lamp Supply Voltage (North America)
0.5 BN/BK | 309 | Right Park Lamp Supply Voltage (Except North America)
11 | 0.5 BN/BK | 309 | Right Park Lamp Supply Voltage
12 | -- | -- | Not Used
13 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
0.5 PK/BK | 1846 | Ignition 1 Voltage (MR-140/Mexico, Japan)
14 | 1.25 WH/BK | 1798 | Headlamp Relay Control
0.3 GY/BK | Headlamp Relay Control (North America)
15 | 0.5 PU/BK | 709 | Left Park Lamp Supply Voltage (Except North America)
0.5 PU/WH | 709 | Left Park Lamp Supply Voltage (North America)
16 | -- | -- | Not Used
17 | 0.5 BK | 28 | Horn Relay Control
18 | 0.3 WH | 1080 | Park Lamp Relay Control
19 | 0.5 YE/D-GN | 317 | Fog Lamp Relay Coil Supply Voltage
20 | 1.25 PU | 12 | Headlamp Low Beam Supply Voltage (Notchback/Station Wagon Except North America)
2 L-BU | 1346 | Headlamp Supply Voltage/ Headlamp Control
21 | -- | -- | Not Used

### Fuse Block - Underhood X2

#### Connector Part Information

- OEM: MG652719
- Service: N/A
- Description: 11-Way F (WH)

#### Fuse Block - Underhood X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.25 PU | 12 | Headlamp Low Beam Supply Voltage
2 | 1.25 L-GN | 11 | Headlamp High Beam Supply Voltage
3 | 0.5 OG/BK | 1340 | Battery Positive Voltage
4 | 2 PU | 293 | Rear Defog Element Supply Voltage
2 PU | 293 | Rear Defog Element Supply Voltage
5 | 2 RD | 581 | Power Window Supply Voltage - Driver Door
6 | 1.25 OG/BK | 540 | Battery Positive Voltage
7 | 0.5 PK | 539 | Ignition 1 Voltage
8 | 0.5 OG/BK | 640 | Battery Positive Voltage
9 | 0.5 OG/BK | 640 | Battery Positive Voltage
0.5 OG | 640 | Battery Positive Voltage (DL7)
10 | 0.5 OG/BK | 640 | Battery Positive Voltage (Hatchback/Notchback)
0.5 OG | 640 | Battery Positive Voltage
11 | 2 OG | 580 | Power Window Supply Voltage

### Fuse Block - Underhood X3

#### Connector Part Information

- OEM: MG65105
- Service: N/A
- Description: 10-Way F 090-II Series (WH)

#### Fuse Block - Underhood X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
0.5 PK/BK | 1846 | Ignition 1 Voltage (2.0L L34)
0.5 PK/WH | 1846 | Ignition 1 Voltage (2.0L Diesel)
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
0.5 PK/BK | 1846 | Ignition 1 Voltage (2.0L L34)
3-4 | -- | -- | Not Used
5 | 0.5 PK/BK | 1846 | Ignition 1 Voltage (Mexico, Japan w/MR-140)
6 | 0.5 BK | 1846 | Ignition 1 Voltage
0.5 PK/BK | 1846 | Ignition 1 Voltage (1.4L, 1.8L, 2.0L Diesel)
7 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
8 | 0.5 PK | 139 | Ignition 1 Voltage (2.0L L34)
0.5 PK | 139 | Ignition 1 Voltage (1.6L, 2.0L L34, 2.0L Diesel)
9 | 0.5 PK | 139 | Ignition 1 Voltage
0.5 PK | 139 | Ignition 1 Voltage
10 | 0.5 PK | 139 | Ignition 1 Voltage
0.5 PK | 139 | Ignition 1 Voltage

### Fuse Block - Underhood X4

#### Connector Part Information

- OEM: MG652503
- Service: N/A
- Description: 24-Way F Hybrid Series (WH)

#### Fuse Block - Underhood X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 309 | Right Park Lamp Supply Voltage (Notchback, Except North America)
2 | 0.5 BN/WH | 309 | Right Park Lamp Supply Voltage (North America)
3 | 0.85 PU | 34 | Fog Lamp Supply Voltage (w/Front Fog Lamp)
4 | 0.5 BN | 990 | Power Steering Pressure Switch Signal (Except North America)
5 | 0.5 D-GN | 59 | A/C Compressor Clutch Coil Supply Voltage (w/Air Conditioning)
6-7 | -- | -- | Not Used
8 | 0.85 PU | 34 | Fog Lamp Supply Voltage (w/Front Fog Lamps)
9 | 0.5 OG | 1240 | Battery Positive Voltage
0.5 OG | 1240 | Battery Positive Voltage
10 | -- | -- | Not Used
11 | 1.25 YE | 712 | Left Headlamp Low Beam Supply Voltage
12 | 2 BK | 50 | Ground
13-14 | -- | -- | Not Used
15 | 2 L-BU | 409 | Cooling Fan Motor Supply Voltage
16 | 1.25 PU | 312 | Right Headlamp Low Beam Supply Voltage
17 | 1.25 L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
18 | 1.25 D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
19 | 0.5 PU | 709 | Left Park Lamp Supply Voltage (North America)
20 | 0.5 PU | 709 | Left Park Lamp Supply Voltage (Notchback) (Except North America)
21 | 2 PU | 532 | Cooling Fan Motor Supply Voltage
22 | 2 PU | 532 | Cooling Fan Motor Supply Voltage
23 | 0.5 D-GN | 29 | Horn Control
0.85 D-GN | 29 | Horn Control (Dual Horn)
24 | -- | -- | Not used

### Fuse Block - Underhood X5

#### Connector Part Information

- OEM: MG651926
- Service: N/A
- Description: 4-Way F 312-II Series (WH)

#### Fuse Block - Underhood X5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 RD | 742 | Battery Positive Voltage
2 | 2 RD/D-BU | 142 | Battery Positive Voltage
3 | 2 RD/D-GN | 1642 | Battery Positive Voltage
4 | 2 RD/WH | 642 | Battery Positive Voltage

### Fuse Block - Underhood X6

#### Connector Part Information

- OEM: MG651080
- Service: N/A
- Description: 20-Way F 090-II Series (WH)

#### Fuse Block - Underhood X6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage
0.5 OG | 440 | Battery Voltage (1.6L, 2.0L L34, 2.0L Diesel))
2 | 0.5 PK | 739 | Ignition 1 Voltage (1.4L/1.8L/2.0L)
1.25 PK | 739 | Ignition 1 Voltage (1.6L)
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
0.5 GY | 120 | Fuel Pump Supply Voltage (1.4L/1.8L/2.0L)
4 | 0.5 D-GN/WH | 335 | Low Speed Cooling Fan Relay Control
0.5 D-GN | 335 | Low Speed Cooling Fan Relay Control (Except North America)
5 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
0.5 D-BU | 473 | High Speed Cooling Fan Relay Control (Dual Fans)
6 | -- | -- | Not Used
7 | 0.5 D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage
0.5 PU/WH | 67 | A/C Compressor Clutch Coil Supply Voltage (1.6L/1.8L)
0.5 PU | 67 | A/C Compressor Clutch Coil Supply Voltage (2.0L Diesel)
8 | 0.5 OG | 440 | Battery Positive Voltage
0.5 OG | 440 | Battery Positive Voltage(1.6L, 2.0L Diesel)
0.5 PK/D-BU | 440 | Battery Positive Voltage(1.6L, 2.0L L34)
9 | 0.5 OG | 440 | Battery Positive Voltage (Except 1.6L)
10 | 0.5 L-GN | 465 | Fuel Pump Relay Control
0.5 D-GN/WH | Fuel Pump Relay Control (1.6L)
11 | -- | -- | Not Used
12 | 0.85 PK/D-BU | 539 | Ignition 1 Voltage
0.5 PK/D-BU | 539 | Ignition 1 Voltage
0.5 PK | 539 | Ignition 1 Voltage (Sirius D4)
13 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage
14 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage (2.0L Diesel)
0.5 PK/BK | 539 | Ignition 1 Voltage (2.0L Diesel)
15 | 0.5 D-BU | 876 | Serial Data (JL9)
16 | -- | -- | Not Used
17 | 1.25 BK | 250 | Ground (2.0L L34)
0.5 D-BU/WH | 471 | Main Relay Control
18 | 0.5 BN | 990 | Power Steering Pressure Switch Signal (Except North America)
19 | 0.5 PK | 139 | Ignition 1 Voltage (HV 240)
0.5 BK | 250 | Ground (MR 140)
0.5 PK/D-BU | 539 | Ignition 1 Voltage (Sirius D4)
20 | -- | -- | Not Used

### Fuse Block - Underhood X7

#### Connector Part Information

- OEM: MG652500
- Service: N/A
- Description: 2-Way F 312-II Series (WH)

#### Fuse Block - Underhood X7

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 4 RD | 42 | Battery Positive Voltage
2 | 4 RD | 42 | Battery Positive Voltage

### Fuse Block - Underhood Auxiliary Label

#### Fuse Block - Underhood Auxiliary Label Usage

No. | Device | Rating | Description
--- | --- | --- | ---
AF1 | Glow Plug Control Unit | 60A | Glow Plug Control Unit
AF2 | Fuel Filter Heater Relay | 30A | Fuel Filter Heater Relay
AF3 | PTC-1 Relay | 40A | PTC-1 Relay
AF4 | PTC-2 Relay | 40A | PTC-2 Relay
AF5 | PTC-3 Relay | 40A | PTC-3 Relay

### Fuse Block - I/P Label

#### Fuse Block - I/P Label Usage

No | Device | Rating | Description
--- | --- | --- | ---
F1 | AIRBAG Fuse | 10A | SDM
F2 | ECM Fuse | 10A | TCM, ECM, Generator, VGIS, VSS
F3 | TRN SIG LAMPS Fuse | 15A | Hazard Switch
F4 | CLSTR, BTSI Fuse | 10A | Cluster, Brake Switch, Chime Bell, Brake Switch, SSPS Module, A/C Control Switch
F5 | -- | -- | Not Used
F6 | ENG FUSE BOX DRL Fuse | 10A | A/C Comp Relay, Defog Relay, Power Window Relay, Headlamp Relay
F7 | HVAC Fuse | 20A | Blower Relay, A/C Control Switch, HVAC
F8 | S/ROOF Fuse | 15A | Electric Mirror Switch, Folding Mirror, Sun Roof Module
F9 | WPR Fuse | 25A | Wiper Motor, Wiper Switch, Rain Sensor Unit - RHD
F10 | AIRBAG Fuse | -- | Occupant Classification Sensor, Clock
F11 | ABS Fuse | 10A | EBCM, Oil Feeding Connector
F12 | IMMOBILIZER Fuse (Except North America) | 10A | Immobilizer, Theft Deterrent Control Unit, Rain Sensor Unit - LHD
F13 | TCM Fuse | 10A | TCM
F14 | HAZARD LAMPS Fuse | 15A | Hazard Switch
F15 | RKE Fuse | 15A | Theft Deterrent Control Unit
F16 | DLC Fuse | 10A | DLC
F17 | RADIO/CLK Fuse | 10A | Clock, Radio
F18 | AUT LTR Fuse | 15A | Extra Power Jack
F19 | LTR Fuse | 15A | Cigar Lighter
F20 | BCK/UP Fuse | 10A | Reverse Lamp Switch, PNP Switch
F21 | BATT SAVERFuse | 15A | Rear Fog Relay
F22 | AUTO A/C Fuse | 15A | Clock, HVAC, A/C Control Switch
F23 | RADIO Fuse | 15A | Radio
F24 | Immobilizer Fuse (Except North America) | 10A | Immobilizer (1.6L and 1.8L)

### Fuse Block - I/P Top View

### Fuse Block - I/P Bottom View

### Fuse Block - I/P

#### Connector Part Information

- OEM: 936195-1
- Service: N/A
- Description: 76-Way F 090/250 Hybrid Series (BK)

#### Fuse Block - I/P

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.25 BN | 441 | Ignition 3 Voltage
2 | 0.3 BK | 250 | Ground
3 | 0.85 PK | 539 | Ignition 1 Voltage (Automatic Transmission)
0.85 PK | 539 | Ignition 1 Voltage (Automatic Transmission)
4 | 2 BK | 250 | Ground
5 | 0.85 PK | 339 | Ignition 1 Voltage
6 | 0.5 PK | 239 | Ignition 1 Voltage
7 | 0.3 PK | 239 | Ignition 1 Voltage (C60/C66)
8 | 0.3 PK | 239 | Ignition 1 Voltage (w/Variable Effort Steering)
9 | 0.3 BK | 250 | Ground
10 | -- | -- | Not Used
11 | 0.5 BN | 141 | Ignition 3 Voltage (T61)
12 | 2 OG | 300 | Ignition 3 Voltage
13 | 1.25 BN | 41 | Ignition 3 Voltage (C68)
14 | 0.5 YE | 317 | Fog Lamp Relay Coil Supply Voltage (T79)
15 | 0.5 YE | 517 | Fog Lamp Relay Coil Supply Voltage (T96)
16 | -- | -- | Not Used
17 | 0.5 PK | 1139 | Ignition 1 Voltage
18 | 0.5 PK | 239 | Ignition 1 Voltage (RHD/ North America)
0.5 OG | 239 | Ignition 1 Voltage (LHD)
19 | 0.5 PK | 239 | Ignition 1 Voltage (Auto Trans w/M97 or Man Trans w/LMN)
20 | 0.3 PK | 239 | Ignition 1 Voltage (w/Alarm)
21 | 0.5 PK | 239 | Ignition 1 Voltage
22 | 0.5 BK | 250 | Ground
23 | -- | -- | Not Used
24 | 0.85 BN | 141 | Ignition 3 Voltage
25 | 0.5 BN | 641 | Ignition 3 Voltage
0.85 BN | 641 | Ignition 3 Voltage
26 | 0.5 YE | 317 | Fog Lamp Relay Coil Supply Voltage (T96)
27 | 1.25 BN | 441 | Ignition 3 Voltage
28 | 0.5 PK | 939 | Ignition 1 Voltage
29 | -- | -- | Not Used
30 | 1.25 PK | 3 | Ignition 1 Voltage
31 | 0.5 PK | 239 | Ignition 1 Voltage
32 | 0.5 PK | 230 | Ignition 1 Voltage
33 | 0.5 OG | 440 | Battery Positive Voltage
34 | 0.85 OG | 1040 | Battery Positive Voltage
35 | 1.25 BN | 41 | Ignition 2 Voltage (C60/C66)
0.85 BN | 41 | Ignition 2 Voltage (C68)
36 | 1.25 OG | 340 | Battery Positive Voltage (UJ9)
1.25 OG | 340 | Battery Positive Voltage
37 | 0.5 OG | 1840 | Battery Positive Voltage
38 | 0.5 YE | 317 | Fog Lamp Relay Coil Supply Voltage (T96)
39 | 0.85 YE | 243 | Ignition 3 Voltage
40 | 1.25 BN | 441 | Ignition 3 Voltage
41 | 1.25 OG | 140 | Battery Positive Voltage (T61)
42 | 1.25 OG | 140 | Battery Positive Voltage
1.25 OG | 140 | Battery Positive Voltage (T61)
43 | 0.5 PK | 739 | Ignition 1 Voltage
44 | 0.5 PK | 639 | Ignition 1 Voltage
45 | 0.5 BK | 250 | Ground (T79)
46 | 0.5 BK | 250 | Ground
47 | 2 RD | 142 | Charge Indicator Control
48 | -- | -- | Not Used
49 | 0.5 L-BU | 20 | Stop Lamp Switch Signal/Stop Lamp Supply Voltage (M97)
50 | 0.5 L-BU | 20 | Stop Lamp Switch Signal/Stop Lamp Supply Voltage (w/Automatic Transmission)
51 | 0.3 YE | 43 | Accessory Voltage
52 | 0.5 YE | 43 | Accessory Voltage (w/Key Interlock)
53 | 0.85 YE | 143 | Accessory Voltage
54 | 0.5 PK | 639 | Ignition 1 Voltage (BAHr)
55 | 0.3 PU/WH | 33 | Brake Warning Indicator Control
0.3 PU/WH | 33 | Brake Warning Indicator Control (North America w/T61)
56 | 0.85 BK | 250 | Ground
57 | 0.5 BK | 250 | Ground (T79)
58 | 0.5 BK | 250 | Ground
59 | -- | -- | Not Used
60 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal (K34)
61 | 1.25 L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
62 | 0.5 YE | 43 | Accessory Voltage (w/Key Interlock)
63 | 0.5 YE | 43 | Accessory Voltage
64 | 2 BN | 4 | Accessory Voltage
65 | 1.25 OG | 140 | Battery Positive Voltage (T61, Except North America)
66 | 0.5 PK | 839 | Ignition 1 Voltage (MFA)
67 | 0.85 PK | 839 | Ignition 1 Voltage
68 | 0.3 PU/WH | 33 | Brake Warning Indicator Lamp
69 | 0.5 BK | 250 | Ground (WU5)
70 | 0.5 BK | 250 | Ground
71 | -- | -- | Not Used
72 | 0.5 OG | 1540 | Battery Positive Voltage
0.5 OG | 1540 | Battery Positive Voltage
0.5 OG | 1540 | Battery Positive Voltage (T79)
73 | 0.5 OG | 1140 | Battery Positive Voltage
74 | 1.25 OG | 40 | Battery Positive Voltage
75 | 0.5 OG | 240 | Battery Positive Voltage (BAH)
76 | 1.25 L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal