For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screw from the rear portion of the floor console.
3. Remove the screws from the front portion of the floor console.
4. Remove the floor console.
5. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the floor console.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front portion of the floor console with the screws.
4. Install the screws to the rear portion of the floor console.
5. Connect the negative battery cable.