For 1990-2009 cars

### Removal Procedure

Notice: Refer to Belt Dressing Notice in the Preface section.

1. Remove the air filter housing assembly bolts and the air intake tube.
2. Remove the air filter housing assembly from the vehicle.
3. Use a wrench to turn the tensioner bolt clockwise, compressing the tensioner and releasing the tension on the serpentine accessory drive belt.
4. Remove the serpentine accessory drive belt.

### Installation Procedure

1. Use a wrench to turn the tensioner bolt clockwise, compressing the tensioner and releasing the tension on the serpentine accessory drive belt.
2. With the wrench in place on the tensioner bolt, loop the serpentine accessory drive belt loosely over the pulleys.
3. Slip the belt over the tensioner.
4. Remove the wrench from the tensioner bolt and the belt will tighten itself.
5. Install the air filter housing assembly into the vehicle

Notice: Refer to Fastener Notice in the Preface section.

6. Install the air intake tube and the air filter housing assembly bolts.

Tighten
Tighten the air filter housing assembly bolts to 6 N·m (53 lb in).