For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
001 |  | SDM | DTC 001
002 |  | SDM | DTC 002
003 |  | SDM | DTC 003
004 |  | SDM | DTC 004
005 |  | SDM | DTC 005
006 |  | SDM | DTC 006
007 |  | SDM | DTC 007
008 |  | SDM | DTC 008
009 |  | SDM | DTC 009
010 |  | SDM | DTC 010
011 |  | SDM | DTC 011
012 |  | SDM | DTC 012
013 |  | SDM | DTC 013
014 |  | SDM | DTC 014
015 |  | SDM | DTC 015
016 |  | SDM | DTC 016
023 |  | SDM | DTC 023
024 |  | SDM | DTC 024
025 |  | SDM | DTC 025
031 |  | SDM | DTC 031
032 |  | SDM | DTC 032
033 |  | SDM | DTC 033
034 |  | SDM | DTC 034
035 |  | SDM | DTC 035
038 |  | SDM | DTC 038
052 |  | SDM | DTC 052
053 |  | SDM | DTC 053
054 |  | SDM | DTC 054
055 |  | SDM | DTC 055
056 |  | SDM | DTC 056
057 |  | SDM | DTC 057
058 |  | SDM | DTC 058
059 |  | SDM | DTC 059
080 |  | SDM | DTC 080
081 |  | SDM | DTC 081
082 |  | SDM | DTC 082
083 |  | SDM | DTC 083
084 |  | SDM | DTC 084
085 |  | SDM | DTC 085
086 |  | SDM | DTC 086
087 |  | SDM | DTC 087
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1104 | Passenger Seat Occupant Classification System (OCS) Voltage Out of Range | SDM | DTC B1104
B1326 | Front End Sensor 1 Short to Ground | SDM | DTC B1326
B1327 | Front End Sensor 1 Short to Battery | SDM | DTC B1327
B1328 | Front End Sensor 1 Internal Electronic Failure | SDM | DTC B1328
B1329 | Front End Sensor 1 Invalid Serial Data Received | SDM | DTC B1329
B1330 | Incorrect Electronic Front End Sensor 1 Installed | SDM | DTC B1330
B1331 | Front End Sensor 2 Short to Ground | SDM | DTC B1331
B1332 | Front End Sensor 2 Short to Battery | SDM | DTC B1332
B1333 | Front End Sensor 2 Internal Electronic Failure | SDM | DTC B1333
B1334 | Front End Sensor 2 Invalid Serial Data Received | SDM | DTC B1334
B1335 | Incorrect Electronic Front End Sensor 2 Installed | SDM | DTC B1335
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Short to Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1440 | Passenger Seat Occupant Classification System (OCS) Circuit Short to Ground | SDM | DTC B1440
B1446 | Passenger Seat Occupant Classification System (OCS) Circuit Short to Battery | SDM | DTC B1446
B1447 | Passenger Seat Occupant Classification System (OCS) Sensor Circuit | SDM | DTC B1447
B1448 | Passenger Seat Occupant Classification System (OCS) Sensor | SDM | DTC B1448
B1449 | Passenger Seat Occupant Classification Sensor Communication | SDM | DTC B1449
B1450 | Incorrect Passenger Seat Occupant Classification Sensor Installed | SDM | DTC B1450
B1481 | Driver Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1481
B1482 | Driver Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1482
B1483 | Driver Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1483
B1484 | Driver Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1484
B1485 | Passenger Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1485
B1486 | Passenger Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1486
B1487 | Passenger Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1487
B1488 | Passenger Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1488
B1620 | ECU Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B1670 | Frontal Stage 2 Deployment Commanded | SDM | DTC B1670
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0040
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0045
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0050
C0060 | Left Front Dump Solenoid Circuit Open | EBCM | DTC C0060/C0065
C0065 | Left Front Hold Valve Circuit Open | EBCM | DTC C0060/C0065
C0070 | Right Front Dump Solenoid Circuit Open | EBCM | DTC C0070/C0075
C0075 | Right Front Hold Valve Circuit Open | EBCM | DTC C0070/C0075
C0080 | Left Rear Dump Solenoid Circuit Open | EBCM | DTC C0080/C0085
C0085 | Left Rear Hold Valve Circuit Open | EBCM | DTC C0080/C0085
C0090 | Right Rear Dump Solenoid Circuit Open | EBCM | DTC C0090/C0095
C0095 | Right Rear Hold Valve Circuit Open | EBCM | DTC C0090/C0095
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0121 | ABS Relay Circuit | EBCM | DTC C0121
C0141 | LF TCS Solenoid/Motor #1 Circuit | EBCM | DTC C0141-C0156
C0146 | LF TCS Solenoid/Motor #2 Circuit | EBCM | DTC C0141-C0156
C0151 | RF TCS Solenoid/Motor #1 Circuit | EBCM | DTC C0141-C0156
C0156 | RF TCS Solenoid/Motor #2 Circuit | EBCM | DTC C0141-C0156
C0161 | Stop Lamp Switch Circuit Open | EBCM | DTC C0161
C0245 | Wheel Speed Signal Malfunction | EBCM | DTC C0245
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0800 | Battery Voltage Out of Range | EBCM | DTC C0800
C0931 | System Thermal High | EBCM | DTC C0931
P0016 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0016 or P0340 for the 1.8L engine or DTC P0016 or P0340 for the 2.0L engine
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030 or P0036 for the 1.4L engine or DTC P0030 or P0036 for the 1.6L engine
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030 or P0036 for the 1.4L engine or DTC P0030 or P0036 for the 1.6L engine
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.4L engine

• | DTC P0107 or P0108 for the 1.6L engine

• | DTC P0107 or P0108 for the 1.8L engine

• | DTC P0107 or P0108 for the 2.0L engine

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.4L engine

• | DTC P0107 or P0108 for the 1.6L engine

• | DTC P0107 or P0108 for the 1.8L engine

• | DTC P0107 or P0108 for the 2.0L engine

P0110 | Intake Air Temperature (IAT) Sensor Circuit | ECM | DTC P0110 or P0111
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0110 or P0111
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.4L engine

• | DTC P0112 or P0113 for the 1.6L engine

• | DTC P0112 or P0113 for the 1.8L engine

• | DTC P0112 or P0113 for the 2.0L engine

P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.4L engine

• | DTC P0112 or P0113 for the 1.6L engine

• | DTC P0112 or P0113 for the 1.8L engine

• | DTC P0112 or P0113 for the 2.0L engine

P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.4L engine

• | DTC P0117 or P0118 for the 1.6L engine

• | DTC P0117 or P0118 for the 1.8L engine

• | DTC P0117 or P0118 for the 2.0L engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.4L engine

• | DTC P0117 or P0118 for the 1.6L engine

• | DTC P0117 or P0118 for the 1.8L engine

• | DTC P0117 or P0118 for the 2.0L engine

P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.4L engine

• | DTC P0122, P0123, P0222, or P0223 for the 1.6L engine

• | DTC P0122 or P0123 for the 1.8L engine

• | DTC P0122 or P0123 for the 2.0L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 2.0L engine

P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.4L engine

• | DTC P0122, P0123, P0222, or P0223 for the 1.6L engine

• | DTC P0122 or P0123 for the 1.8L engine

• | DTC P0122 or P0123 for the 2.0L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 2.0L engine

P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM |

• | DTC P0131 or P0132 for the 1.4L engine

• | DTC P0131 or P0137 for the 1.6L engine

• | DTC P0131 or P0132 for the 1.8L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine

P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM |

• | DTC P0131 or P0132 for the 1.4L engine

• | DTC P0132 or P0138 for the 1.6L engine

• | DTC P0131 or P0132 for the 1.8L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine

P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM |

• | DTC P0133 for the 1.4L engine

• | DTC P0133 for the 1.6L engine

• | DTC P0133, P1133, or P1134 for the 1.8L engine

• | DTC P0133 or P0139 for the 2.0L engine

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM | DTC P0134 or P0140 for the 1.8L engine or DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine
P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0135 or P0141 for the 1.4L engine

• | DTC P0135 or P0141 for the 1.6L engine

• | DTC P0135 or P0141 for the 1.8L engine

• | DTC P0135 or P0141 for the 2.0L engine

P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM |

• | DTC P0137 or P0138 for the 1.4L engine

• | DTC P0131 or P0137 for the 1.6L engine

• | DTC P0137 or P0138 for the 1.8L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine

P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM |

• | DTC P0137 or P0138 for the 1.4L engine

• | DTC P0132 or P0138 for the 1.6L engine

• | DTC P0137 or P0138 for the 1.8L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine

P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0133 or P0139
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM |

• | DTC P0140 for the 1.4L engine

• | DTC P0140 for the 1.6L engine

• | DTC P0134 or P0140 for the 1.8L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.0L engine

P0141 | HO2S Heater Performance Sensor 2 | ECM |

• | DTC P0135 or P0141 for the 1.4L engine

• | DTC P0135 or P0141 for the 1.6L engine

• | DTC P0135 or P0141 for the 1.8L engine

• | DTC P0135 or P0141 for the 2.0L engine

P0171 | Fuel Trim System Lean | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0171 or P0172 for the 1.6L engine

• | DTC P0171 or P0172 for the 1.8L engine

• | DTC P0171, P0172, P2187, or P2188 for the 2.0L engine

P0172 | Fuel Trim System Rich | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0171 or P0172 for the 1.6L engine

• | DTC P0171 or P0172 for the 1.8L engine

• | DTC P0171, P0172, P2187, or P2188 for the 2.0L engine

P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, or P0204
P0217 | Engine Coolant Over Temperature | ECM | DTC P0217
P0218 | Transmission Over Temperature Condition | TCM | DTC P0218
P0222 | Idle Speed Control (ISC) Motor Position Sensor Circuit Low Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.4L engine

• | DTC P0122, P0123, P0222, or P0223 for the 1.6L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 2.0L engine

P0223 | Idle Speed Control (ISC) Motor Position Sensor Circuit High Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.4L engine

• | DTC P0122, P0123, P0222, or P0223 for the 1.6L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 2.0L engine

P0261 | Injector 1 Control Circuit Low Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0262 | Injector 1 Control Circuit High Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0264 | Injector 2 Control Circuit Low Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0265 | Injector 2 Control Circuit High Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0267 | Injector 3 Control Circuit Low Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0268 | Injector 3 Control Circuit High Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0270 | Injector 4 Control Circuit Low Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0271 | Injector 4 Control Circuit High Voltage | ECM |

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.4L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine

• | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.0L engine

P0300 | Engine Misfire Detected | ECM |

• | DTC P0300 for the 1.4L engine

• | DTC P0300 for the 1.6L engine

• | DTC P0300-P0304 for the 1.8L engine

• | DTC P0300-P0304 for the 2.0L engine

P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 for the 1.8L engine or DTC P0300-P0304 for the 2.0L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 for the 1.8L engine or DTC P0300-P0304 for the 2.0L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 for the 1.8L engine or DTC P0300-P0304 for the 2.0L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 for the 1.8L engine or DTC P0300-P0304 for the 2.0L engine
P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315 for the 1.8L engine or DTC P0315 for the 2.0L engine
P0317 | Rough Road Sensing System Input Not Present | ECM | DTC P0317 for the 1.8L engine or DTC P0317 for the 2.0L engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 1.8L engine or DTC P0324 for the 2.0L engine
P0325 | Knock Sensor (KS) Circuit | ECM | DTC P0325 for the 1.8L engine or DTC P0325 for the 2.0L engine
P0327 | Knock Sensor (KS) Circuit Low Frequency | ECM | DTC P0327 for the 1.4L engine or DTC P0327 for the 1.6L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335, P0336, or P0337 for the 1.4L engine

• | DTC P0335, P0336, or P0337 for the 1.6L engine

• | DTC P0335 or P0336 for the 1.8L engine

• | DTC P0335, P0336, or P0337 for the 2.0L engine

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335, P0336, or P0337 for the 1.4L engine

• | DTC P0335, P0336, or P0337 for the 1.6L engine

• | DTC P0335 or P0336 for the 1.8L engine

• | DTC P0335, P0336, or P0337 for the 2.0L engine

P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM | DTC P0335, P0336, or P0337 for the 1.4L engine or DTC P0335, P0336, or P0337 for the 1.6L engine
P0341 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 or P0342 for the 1.4L engine or DTC P0341 or P0342 for the 1.6L engine
P0342 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0341 or P0342 for the 1.4L engine or DTC P0341 or P0342 for the 1.6L engine
P0351 | Ignition Coil 1 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.4L engine

• | DTC P0351 or P0352 for the 1.6L engine

• | DTC P0351 or P0352 for the 1.8L engine

• | DTC P0351 or P0352 for the 2.0L engine

P0352 | Ignition Coil 2 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.4L engine

• | DTC P0351 or P0352 for the 1.6L engine

• | DTC P0351 or P0352 for the 1.8L engine

• | DTC P0351 or P0352 for the 2.0L engine

P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.8L engine

• | DTC P0400, P0401, P0402, or P1402 for the 2.0L engine

P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.8L engine

• | DTC P0400, P0401, P0402, or P1402 for the 2.0L engine

P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.8L engine

• | DTC P0400, P0401, P0402, or P1402 for the 2.0L engine

P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.8L engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 2.0L engine

P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.8L engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 2.0L engine

P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.8L engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 2.0L engine

P0420 | Catalyst System Low Efficiency Bank 1 | ECM |

• | DTC P0420 for the 1.4L engine

• | DTC P0420 for the 1.6L engine

• | DTC P0420 for the 1.8L engine

• | DTC P0420 for the 2.0L engine

P042E | Exhaust Gas Recirculation (EGR ) Closed Position | ECM | DTC P0404-P0406, P042E, or P1404 for the 1.8L engine
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443
P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0444 or P0445 for the 1.4L engine or DTC P0444 or P0445 for the 1.6L engine
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445 for the 1.4L engine or DTC P0444 or P0445 for the 1.6L engine
P0446 | Evaporative Emissions (EVAP) Vent System Performance | ECM | DTC P0446
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451 or P0454
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451 or P0454
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0458 or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0458 or P0459
P0488 | Exhaust Gas Recirculation (EGR) Closed Valve Pintle Error | ECM | DTC P0122, P0123, P0222, P0223, or P2135
P0496 | Evaporative Emissions (EVAP) System Continuous Purge Flow | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Open | ECM | DTC P0498 or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Shorted | ECM | DTC P0498 or P0499
P0501 | Vehicle Speed Sensor (VSS) Performance | ECM | DTC P0501 for the 1.4L engine or DTC P0501 for the 1.6L engine
P0502 | Vehicle Speed Sensor (VSS) Circuit | ECM | DTC P0502 for the 1.8L engine or DTC P0502 for the 2.0L engine
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507 for the 1.8L engine or DTC P0506 or P0507 for the 2.0L engine
P0507 | Idle Speed High | ECM | DTC P0506 or P0507 for the 1.8L engine or DTC P0506 or P0507 for the 2.0L engine
P0510 | Idle Speed Control (ISC) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0510 for the 1.4L engine or DTC P0510 for the 1.6L engine
P0562 | System Voltage Low | TCM | DTC P0562 for the Aisin (81-40LE) transmission or DTC P0562 for the ZF 4HP 16 transmission
P0563 | System Voltage High | TCM | DTC P0563 for the Aisin (81-40LE) transmission or DTC P0563 for the ZF 4HP 16 transmission
P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0601 | Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0603 | Internal Control Module Keep Alive Memory (KAM) Error | TCM | DTC P0603
P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0604 | Control Module Random Access Memory (RAM) | TCM | DTC P0604 for the Aisin (81-40LE) transmission or DTC P0604 for the ZF 4HP 16 transmission
P0605 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0606 | Transaxle Control Module Processor Fault - Failure of External Watchdog | TCM | DTC P0606
P0607 | Control Module Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629 for the 1.4L engine or DTC P0628 or P0629 for the 1.6L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629 for the 1.4L engine or DTC P0628 or P0629 for the 1.6L engine
P0630 |  | ECM | DTC P0630
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641 or P0651
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM |

• | DTC P0650 or P1650 for the 1.4L engine

• | DTC P0650 or P1650 for the 1.6L engine

• | DTC P0650 for the 2.0L engine

P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641 or P0651
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660
P0661 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0661 or P0662 for the 1.4L engine or DTC P0660, P0661, or P0662 for the 1.6L engine
P0662 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage | ECM | DTC P0661 or P0662 for the 1.4L engine or DTC P0660, P0661, or P0662 for the 1.6L engine
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 1.4L engine

• | DTC P0700 for the 1.6L engine

• | DTC P0700 for the 1.8L engine

• | DTC P0700 for the 2.0L engine

P0703 | Brake Switch Circuit Malfunction | TCM | DTC P0703
P0705 | Transmission Range Sensor Circuit | TCM | DTC P0705 for the Aisin (81-40LE) transmission or DTC P0705 for the ZF 4HP 16 transmission
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706
P0710 | Transmission Fluid Temperature Sensor Circuit Malfunction | TCM | DTC P0710
P0712 | Transmission Fluid Temperature (TFT) Sensor Low Input | TCM | DTC P0712
P0713 | Transmission Fluid Temperature (TFT) Sensor High Input | TCM | DTC P0713
P0715 | Input Speed Sensor Circuit Malfunction | TCM | DTC P0715
P0716 | Input Speed Sensor Circuit Fault | TCM | DTC P0716
P0717 | Input Speed Sensor - No Signal | TCM | DTC P0717 for the Aisin (81-40LE) transmission or DTC P0717 for the ZF 4HP 16 transmission
P0720 | Output Speed Sensor Circuit Malfunction | TCM | DTC P0720
P0721 | Output Speed Sensor Circuit Fault | TCM | DTC P0721
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0722 for the Aisin (81-40LE) transmission or DTC P0722 for the ZF 4HP 16 transmission
P0725 | Engine Speed Input Circuit Malfunction | TCM | DTC P0725
P0726 | Engine Speed Input Circuit Fault | TCM | DTC P0726
P0727 | Engine Speed Signal Circuit | TCM | DTC P0727 for the Aisin (81-40LE) transmission or DTC P0727 for the ZF 4HP 16 transmission
P0731 | Incorrect 1st Gear Ratio | TCM | DTC P0731
P0732 | Incorrect 2nd Gear Ratio | TCM | DTC P0732
P0733 | Incorrect 3rd Gear Ratio | TCM | DTC P0733
P0734 | Incorrect 4th Gear Ratio | TCM | DTC P0734
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch Circuit Stuck On | TCM | DTC P0742
P0743 | Torque Converter Clutch Circuit Electrical | TCM | DTC P0743
P0748 | Pressure Control Solenoid Electrical | TCM | DTC P0748
P0751 | Shift Solenoid 1 Performance or Stuck Off | TCM | DTC P0751
P0753 | Shift Solenoid 1 Electrical | TCM | DTC P0753
P0756 | Shift Solenoid (SS) 2 Performance Stuck Off | TCM | DTC P0756
P0758 | Shift Solenoid 2 Electrical | TCM | DTC P0758
P0781 | 1-2 Shift Malfunction | TCM | DTC P0781
P0782 | 2-3 Shift Malfunction | TCM | DTC P0782
P0783 | 3-4 Shift Malfunction | TCM | DTC P0783
P0785 | Shift Timing Solenoid | TCM | DTC P0785
P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | ECM | DTC P1106 or P1107
P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | ECM | DTC P1106 or P1107
P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM | DTC P1111 or P1112
P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage | ECM | DTC P1111 or P1112
P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | ECM | DTC P1114 or P1115
P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | ECM | DTC P1114 or P1115
P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage | ECM | DTC P1121 or P1122
P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | ECM | DTC P1121 or P1122
P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1137 or P1166
P1138 | HO2S Circuit High Voltage During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1138 or P2297
P1166 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2 | ECM | DTC P1166 for the 1.8L engine or DTC P1137 or P1166 for the 2.0L engine
P1181 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage | ECM | DTC P1181 or P1182 for the 1.4L engine or DTC P1181 or P1182 for the 1.6L engine
P1182 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage | ECM | DTC P1181 or P1182 for the 1.4L engine or DTC P1181 or P1182 for the 1.6L engine
P1230 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P1230 or P1231 for the 1.4L engine or DTC P1230 or P1231 for the 1.6L engine
P1231 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P1230 or P1231 for the 1.4L engine or DTC P1230 or P1231 for the 1.6L engine
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320 for the 1.4L engine or DTC P1320 for the 1.6L engine
P1321 | Crankshaft Position (CKP) Reluctor Wheel Performance | ECM | DTC P1321 for the 1.4L engine or DTC P1321 for the 1.6L engine
P1382 | Wheel Speed Sensor Circuit Performance | ECM | DTC P1382 or P1385 for the 1.4L engine or DTC P1382 or P1385 for the 1.6L engine
P1385 | Wheel Speed Sensor Circuit | ECM | DTC P1382 or P1385 for the 1.4L engine or DTC P1382 or P1385 for the 1.6L engine
P1390 | Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396 for the 1.4L engine or DTC P1390 or P1396 for the 1.6L engine
P1391 | Rough Road Sensor Performance | ECM | DTC P1391, P1392, or P1393 for the 1.8L engine or DTC P1391, P1392, or P1393 for the 2.0L engine
P1392 | Rough Road Sensor Circuit Low Voltage | ECM | DTC P1391, P1392, or P1393 for the 1.8L engine or DTC P1391, P1392, or P1393 for the 2.0L engine
P1393 | Rough Road Sensor Circuit High Voltage | ECM | DTC P1391, P1392, or P1393 for the 1.8L engine or DTC P1391, P1392, or P1393 for the 2.0L engine
P1396 | Wheel Speed Sensor Circuit w/o ABS | ECM |

• | DTC P1390 or P1396 for the 1.4L engine

• | DTC P1390 or P1396 for the 1.6L engine

• | DTC P1396 or P1397 for the 1.8L engine

• | DTC P1396 or P1397 for the 2.0L engine

P1397 | Wheel Speed Sensor Circuit w/ABS | ECM | DTC P1396 or P1397 for the 1.8L engine or DTC P1396 or P1397 for the 2.0L engine
P1402 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0171 or P0172 for the 1.4L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.8L engine

• | DTC P0400, P0401, P0402, or P1402 for the 2.0L engine

P1403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine or DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine
P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.4L engine

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.6L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.8L engine

P1476 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Short to Voltage | ECM | DTC P1476, P1477, or P1478 for the 1.4L engine or DTC P1476, P1477, or P1478 for the 1.6L engine
P1477 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Short to Ground | ECM | DTC P1476, P1477, or P1478 for the 1.4L engine or DTC P1476, P1477, or P1478 for the 1.6L engine
P1478 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Open | ECM | DTC P1476, P1477, or P1478 for the 1.4L engine or DTC P1476, P1477, or P1478 for the 1.6L engine
P1504 | Transmission Control Module (TCM) Communication Performance | ECM | DTC P1504 for the 1.4L engine or DTC P1504 for the 1.6L engine
P1511 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P1511, P1512, or P1513 for the 1.4L engine or DTC P1511, P1512, or P1513 for the 1.6L engine
P1512 | Idle Speed Control (ISC) System | ECM | DTC P1511, P1512, or P1513 for the 1.4L engine or DTC P1511, P1512, or P1513 for the 1.6L engine
P1513 | Idle Speed Control (ISC) System Performance | ECM | DTC P1511, P1512, or P1513 for the 1.4L engine or DTC P1511, P1512, or P1513 for the 1.6L engine
P1516 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119
P1601 | Lost Communication with TCM | ECM | DTC P1601
P1604 | Data Check of Internal and Extended Ram Failed | TCM | DTC P1604
P1606 | Transaxle Control Module Processor Fault - Reset Counter Error | TCM | DTC P1606
P1606 | Failure of External Watchdog | TCM | DTC P1606
P1607 | Control Module Performance | ECM | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine
P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611 for the 1.4L engine or DTC P1610 or P1611 for the 1.6L engine
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611 for the 1.4L engine or DTC P1610 or P1611 for the 1.6L engine
P1650 | Control Module Performance | ECM |

• | DTC P0650 or P1650 for the 1.4L engine

• | DTC P0650 or P1650 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

P1655 | Control Module Performance | ECM | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine
P1660 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1660 or P1661 for the 1.4L engine or DTC P1660 or P1661 for the 1.6L engine
P1661 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1660 or P1661 for the 1.4L engine or DTC P1660 or P1661 for the 1.6L engine
P1671 | CAN Transmit Message Failure | TCM | DTC P1671
P1672 | CAN Bus OFF Failure | TCM | DTC P1672
P1673 | Can Receive ECM Message Failure | TCM | DTC P1673
P1680 |  | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P1681 |  | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P1683 |  | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

P1779 | Engine Torque Input Signal Malfunction | TCM | DTC P1779
P1780 | Engine Torque Reduction Fault | TCM | DTC P1780
P1781 | Engine Torque Signal Error | TCM | DTC P1781
P1791 | Throttle Position (TP) Sensor Circuit | TCM | DTC P1791 for the Aisin (81-40LE) transmission or DTC P1791 for the ZF 4HP 16 transmission
P1792 | Engine Coolant Signal | TCM | DTC P1792
P1839 | PCS3 Output Shorted To Ground | TCM | DTC P1839
P1840 | PCS3 Output Shorted To Power | TCM | DTC P1840
P1841 | PCS3 Output Open | TCM | DTC P1841
P1850 | Solenoid 1 Output Shorted To Ground | TCM | DTC P1850
P1851 | Solenoid 1 Output Shorted To Power | TCM | DTC P1851
P1852 | Solenoid 1 Output Open | TCM | DTC P1852
P1853 | Solenoid 2 Output Shorted To Ground | TCM | DTC P1853
P1853 | PCS6 Output Shorted To Power | TCM | DTC P1853
P1854 | Solenoid 2 Output Shorted To Power | TCM | DTC P1854
P1855 | Solenoid 2 Output Open | TCM | DTC P1855
P1861 | PCS4 Output Shorted To Ground | TCM | DTC P1861
P1862 | PCS4 Output Shorted To Power | TCM | DTC P1862
P1863 | PCS4 Output Open | TCM | DTC P1863
P1864 | PCS5 Output Shorted To Ground | TCM | DTC P1864
P1865 | PCS5 Output Shorted To Power | TCM | DTC P1865
P1869 | PCS6 Output Open | TCM | DTC P1869
P1871 | PCS Valve Power Supply Circuit Shorted To Power | TCM | DTC P1871
P1874 | Solenoid Valve Power Supply Circuit Shorted To Power | TCM | DTC P1874
P1881 | 2-1 Shift Malfunction | TCM | DTC P1881
P1883 | 3-2 Shift Malfunction | TCM | DTC P1883
P1884 | 4-3 Shift Malfunction | TCM | DTC P1884
P1885 | 3-1 Shift Malfunction | TCM | DTC P1885
P1886 | 4-2 Shift Malfunction | TCM | DTC P1886
P2101 | Idle Speed Control (ISC) Motor Control Circuit | ECM |

• | DTC P2101, P2118, or P2119 for the 1.4L engine

• | DTC P2101, P2118, or P2119 for the 1.6L engine

• | DTC P1516, P2101, or P2119 for the 2.0L engine

P2104 | Throttle Actuator Control (TAC) System - Forced Engine Idle | ECM | DTC P2104, P2105, P2106, or P2110
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2104, P2105, P2106, or P2110
P2106 | Throttle Control System Performance - Throttle Limitation Active | ECM | DTC P2104, P2105, P2106, or P2110
P2110 | Throttle Actuator Control (TAC) System - Forced Limited Engine Speed | ECM | DTC P2104, P2105, P2106, or P2110
P2118 | Idle Speed Control (ISC) System | ECM | DTC P2101, P2118, or P2119 for the 1.4L engine or DTC P2101, P2118, or P2119 for the 1.6L engine
P2119 | Idle Speed Control (ISC) System Performance | ECM |

• | DTC P2101, P2118, or P2119 for the 1.4L engine

• | DTC P2101, P2118, or P2119 for the 1.6L engine

• | DTC P1516, P2101, or P2119 for the 2.0L engine

P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2282 | Intake Manifold Air Leak | ECM | DTC P2282
P2297 | HO2S Circuit High Voltage During Decel Fuel Cut-Off (DFCO) Sensor 2 | ECM | DTC P2297 for the 1.8L or DTC P1138 or P2297 for the 2.0L engine
P2610 | Control Module Ignition Off Timer Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.8L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.0L engine

U0100 | Lost Communication with engine control module (ECM) / transmission control module (TCM) | ECM/TCM | DTC U0100-U0299
U0167 | Lost Communication with Vehicle Immobilizer Control Module | ECM | DTC U0100-U0299
U2105 | CAN Bus Error | TCM | DTC U2105