For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel under cover.
3. Remove the bolts and the daytime running lamp module.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the daytime running lamp module with the bolts and tighten to 2 N·m (18 lb in).
3. Install the instrument panel under cover.
4. Connect the negative battery cable.